For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Transfer Case Input Shaft Seal - Right Notice: Do not use a screwdriver or punch to remove the seal. Using a screwdriver or punch to remove the seal may damage the aluminum housing sealing surface.

#### Special Tools

• | DT-48074 Input and Output Shaft Seal Installer

• | J 8092 Driver Handle

• | J 26941 Bushing and Bearing Remover - 3-4 in

• | J 45124 Removal Bridge