For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the park brake shoes. Refer to Parking Brake Shoe Replacement.

1 | Park Brake Cable Eye

#### Procedure

Disconnect the park brake cable eye from the actuator lever.

2 | Parking Brake Actuator

#### Procedure

Adjust the park brake. Refer to Park Brake Adjustment.