For 1990-2009 cars

Checks | Actions
--- | ---
Check for a stuck concentric slave cylinder. | Replace the concentric slave cylinder. Refer to Clutch Concentric Actuator Cylinder Replacement .
Check for improper return of clutch oil. | Perform the air bleeding. Refer to Hydraulic Clutch Bleeding .
Check for a worn clutch disc or oil contamination. | Replace the necessary clutch components. Refer to Clutch Assembly Replacement .
Check for a warped pressure plate. | Replace the necessary clutch components.