For 1990-2009 cars

Connector 1: | Rear Window Defogger Grid X1
Connector 2: | Rear Window Defogger Grid X2
Connector 3: | Window Motor - Driver
Connector 4: | Window Motor - Passenger
Connector 5: | Window Switch - Driver
Connector 6: | Window Switch - Passenger

### Rear Window Defogger Grid X1

#### Connector Part Information

- OEM: 12004267
- Description: 1-Way F 56 Series Lock Type (BK)

#### Rear Window Defogger Grid X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1.0 BK | 293 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid X2

#### Connector Part Information

- OEM: 12004267
- Description: 1-Way F 56 Series Lock Type (BK)

#### Rear Window Defogger Grid X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1.0 BK | 850 | Ground

### Window Motor - Driver

#### Connector Part Information

- OEM: 12129487
- Description: 2-Way F Metri-Pack Series, Flexlock, Sealed (GY)

#### Window Motor - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 3.0 BN | 165 | Power Window Motor Left Front Down Control
B | 3.0 D-BU | 164 | Power Window Motor Left Front Up Control

### Window Motor - Passenger

#### Connector Part Information

- OEM: 12129487
- Description: 2-Way F Metri-Pack 280 Series, FlexLock, Sealed (GY)

#### Window Motor - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 3.0 BN | 667 | Power Window Motor Right Front Down Control
B | 3.0 D-BU | 666 | Power Window Motor Right Front Up Control

### Window Switch - Driver

#### Connector Part Information

- OEM: 15449340
- Description: 8-Way F GT 280 (BK)

#### Window Switch - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 0.35 GY | 8 | Instrument Panel Lamp Supply
C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 2.0 BK | 550 | Ground
G | 3.0 D-BU | 164 | Power Window Motor Left Front Up Control
H | 3.0 BN | 165 | Power Window Motor Left Front Down Control

### Window Switch - Passenger

#### Connector Part Information

- OEM: 12192825
- Description: 8-Way F Metri-Pack 280 Series (BN)

#### Window Switch - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 0.35 BK | 550 | Ground
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 3.0 BN | 667 | Power Window Motor Right Front Down Control
G | 3.0 D-BU | 666 | Power Window Motor Right Front Up Control
H | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal