For 1990-2009 cars

### Remote Control Door Lock Receiver Replacement

If the remote control door lock receiver is replaced, the following procedures must be performed:

1. Keyless Entry Transmitter Programming--Refer to Transmitter Programming.
2. Setup New RCDLR:

2.1. | Select Remote Control Door Lock Receiver under Module Setup in the scan tool Vehicle Control System menu.

2.2. | Select Setup New RCDLR.

2.3. | Follow the on-sceen instructions.