For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Power Steering Fluid Reservoir Outlet Hose Clamp (Qty: 2)

#### Procedure

Drain as much power steering fluid from the remote power steering fluid reservoir as possible.

2 | Power Steering Fluid Reservoir Outlet Hose

#### Procedure

Fill and bleed the power steering System. Refer to Power Steering System Bleeding .

Tip
When removing or installing the power steering fluid reservoir hose make sure that the it is properly routed and not twisted.