For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate capacities are given in English and metric conversions. Please refer to Recommended Fluids and Lubricantsfor more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant R134a | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer/retailer for more information.
Cooling System | 9.5 qt | 9.0 L
Engine Oil with Filter | 5.0 qt | 4.7 L
Fuel Tank | 13.6 gal | 51.5 L
Transmission, Manual (Complete Drain and Refill) | 2.75 qt | 2.6 L
Wheel Nut Torque | 100 lb ft | 140 N·m
All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual.

#### Engine Specifications

Engine | VIN Code | Transmission | Spark Plug Gap
--- | --- | --- | ---
2.0L L4 | X | Manual | 0.035 in (0.90 mm)