For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Clutch | At the left front corner of the engine, behind the A/C compressor pulley, part of the A/C compressor | Powertrain Component Views | Component Connector End Views
A/C Refrigerant Pressure Sensor | At the top left side of the engine, near the throttle body | Powertrain Component Views | Component Connector End Views
Accelerator Pedal Position (APP) Sensor | Under the left side of the instrument panel, on the accelerator pedal bracket | Powertrain Component Views | Component Connector End Views
Accessory Power Outlet | Lower center of instrument panel, to the right of radio | Instrument Panel/Center Console Component Views | Component Connector End Views
Air Temperature Actuator - Left | In the center of the instrument panel, at the left side of the HVAC module | Instrument Panel/Center Console Component Views | Component Connector End Views
Air Temperature Actuator - Right | In the center of the instrument panel, at the right side of the HVAC module | Instrument Panel/Center Console Component Views | Component Connector End Views
Audio Amplifier (UQ3) | In the passenger compartment, behind the left seat, under body trim panel | Passenger Compartment/Roof Component Views | Component Connector End Views
Battery | In the engine compartment, at the right rear corner, near the underhood fuse block | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Backup Lamp | At the rear of the vehicle, center of the rear bumper fascia | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Backup Lamp Switch | Under the vehicle, at the upper right side of the transmission | Powertrain Component Views | Component Connector End Views
Blower Motor | At the right side of the instrument panel, behind the instrument panel compartment | Instrument Panel/Center Console Component Views | Component Connector End Views
Blower Motor High Speed Relay | At the right side of the instrument panel, behind the instrument panel compartment and in front of the blower motor | Instrument Panel/Center Console Component Views | Component Connector End Views
Blower Motor Resistor | At the right side of the instrument panel, behind instrument panel compartment and below the blower motor | Instrument Panel/Center Console Component Views | Component Connector End Views
Body Control Module (BCM) | At the right side of the instrument panel, under carpet in footwell area | Instrument Panel/Center Console Component Views | Electrical Center Identification Views
Brake Booster Vacuum Sensor | Front of the engine compartment, near the brake fluid level switch and windshield washer fluid pump | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Brake Booster Pump Motor | Front of the engine compartment, near the brake fluid level switch and windshield washer fluid pump | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Brake Fluid Level Switch | At the left rear of the engine compartment, at the base of the brake fluid reservoir | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Brake Pedal Position (BPP) Sensor | Under the left side of the instrument panel, at the top of the brake pedal lever | Instrument Panel/Center Console Component Views | Component Connector End Views
Brake Pressure Modulator Valve (BPMV) | At the left side of the engine compartment, mounted on the inner frame rail, attached to the electronic brake control module (EBCM) | Front of Vehicle/Engine Compartment Component Views | --
Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust | On the top front of the engine, to the left of the ignition coil 1 | Powertrain Component Views | Component Connector End Views
Camshaft Position (CMP) Actuator Solenoid Valve - Intake | On the top rear of the engine to the left of the ignition coil 1 | Powertrain Component Views | Component Connector End Views
Camshaft Position (CMP) Sensor - Exhaust | On the engine, at the top right rear | Powertrain Component Views | Component Connector End Views
Camshaft Position (CMP) Sensor - Intake | On the engine, at the top left rear | Powertrain Component Views | Component Connector End Views
Center High Mounted Stop Lamp (CHMSL) | At the rear of the vehicle, above the license lamp | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Cigar Lighter | In the driver door panel, below the door lock switch | Door Component Views | Component Connector End Views
Clutch Pedal Position (CPP) Sensor | Under the left side of the instrument panel, mounted at the top of the clutch pedal bracket | Instrument Panel/Center Console Component Views | Component Connector End Views
Courtesy/Reading Lamps - Left Front | Located on the Inside Rear View Mirror - Left side | Instrument Panel/Center Console Component Views | --
Courtesy/Reading Lamps - Right Front | Located on the Inside Rear View Mirror - Right side | Instrument Panel/Center Console Component Views | --
Crankshaft Position (CKP) Sensor | At the left rear corner of the engine block, below the starter | Powertrain Component Views | Component Connector End Views
Data Link Connector (DLC) | Under the left side of the instrument panel, near the base of the steering column | Instrument Panel/Center Console Component Views | Splice Pack Connector End Views
Data Link Resistor | Behind the left side of the instrument panel, taped to the instrument panel wiring harness | Instrument Panel/Center Console Component Views | Splice Pack Connector End Views
Door Lock Actuator - Driver (AU3) | Inside the left door, at the center rear | Door Component Views | Component Connector End Views
Door Lock Actuator - Passenger (AU3) | Inside the right door, at the center rear | Door Component Views | Component Connector End Views
Door Lock Switch - Driver (AU3) | In the driver door panel above the radio speaker | Door Component Views | Component Connector End Views
Door Lock Switch - Passenger (AU3) | In the passenger door panel above the radio speaker | Door Component Views | Component Connector End Views
Electronic Brake Control Module (EBCM) | At the left side of the engine compartment, mounted on the inner frame rail | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Engine Control Module (ECM) | At the left rear corner of the engine compartment, near the brake master cylinder and engine coolant overflow reservoir | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Engine Coolant Level Switch | At the left rear corner of the engine compartment, next to the brake master cylinder, at the base of the engine coolant overflow reservoir | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Engine Coolant Temperature (ECT) Sensor | On the engine block, at the left rear corner | Powertrain Component Views | Component Connector End Views
Engine Cooling Fan | At the front of the engine compartment, behind the radiator | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Engine Oil Pressure (EOP) Switch | On the engine, at the lower left corner near the starter | Powertrain Component Views | Component Connector End Views
Evaporative Emission (EVAP) Canister Purge Solenoid Valve | At the top left rear corner of the engine, top rear of engine on the left hand side | Powertrain Component Views | Component Connector End Views
Evaporative Emission (EVAP) Canister Vent Solenoid Valve | At the rear of the fuel tank | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Evaporator Temperature Sensor | Behind the right instrument panel storage compartment to the left side | Instrument Panel/Center Console Component Views | Component Connector End Views
Fog Lamp - Left Front | In the left side of the front bumper | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fog Lamp - Right Front | In the right side of the front bumper | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fog Lamp - Rear | In the center of the rear bumper | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Fog Lamp Switch - Front | To the left of the steering column, in the knee bolster | Instrument Panel/Center Console Component Views | Component Connector End Views
Fog Lamp Switch - Rear | To the left of the steering column, in the knee bolster | Instrument Panel/Center Console Component Views | Component Connector End Views
Folding Top Cover Actuator | Outside of the vehicle at the base of the rear window behind the drivers seat | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Fuel Injector 1 | On the left side of the engine, attached to the fuel rail at the number 1 cylinder | Powertrain Component Views | Component Connector End Views
Fuel Injector 2 | On the left side of the engine, attached to the fuel rail at the number 2 cylinder | Powertrain Component Views | Component Connector End Views
Fuel Injector 3 | On the left side of the engine, attached to the fuel rail at the number 3 cylinder | Powertrain Component Views | Component Connector End Views
Fuel Injector 4 | On the left side of the engine, attached to the fuel rail at the number 4 cylinder | Powertrain Component Views | Component Connector End Views
Fuel Pump and Sender Assembly | Under the rear of the vehicle, inside the fuel tank | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Fuel Rail Pressure (FRP) Sensor | Top left of engine, on fuel rail, near fuel injector 1 | Powertrain Component Views | Component Connector End Views
Fuel Tank Pressure (FTP) Sensor | Under the rear of the vehicle, connected to the fuel pump and sender assembly | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Fuse Block - Underhood | In the right rear corner of the engine compartment | Front of Vehicle/Engine Compartment Component Views | Electrical Center Identification Views
Generator | At the left front of the engine | Powertrain Component Views | Component Connector End Views
Hazard Warning Switch | Center of the instrument panel between A/C vents | Instrument Panel/Center Console Component Views | Component Connector End Views
Headlamp - Left High Beam | Part of the left headlamp assembly, at the left front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Headlamp - Left Low Beam | Part of the right headlamp assembly, at the right front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Headlamp - Right High Beam | Part of the left headlamp assembly, at the left front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Headlamp - Right Low Beam | Part of the right headlamp assembly, at the right front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Heated Oxygen Sensor (HO2S) 1 | At the rear of the engine compartment, mounted to the exhaust manifold, just above the catalytic converter | Powertrain Component Views | Component Connector End Views
Heated Oxygen Sensor (HO2S) 2 | Under the vehicle, on the exhaust pipe just past the catalytic converter | Powertrain Component Views | Component Connector End Views
High Pressure Fuel Pump | Top left of engine, on fuel rail, near fuel injector 4 | Powertrain Component Views | Component Connector End Views
Horn - Left | At the left front corner of the engine compartment, attached to the hinge bracket | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Horn - Right | At the right front corner of the engine compartment, attached to the hinge bracket | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Horn Switch | Part of the steering wheel assembly, under the inflatable restraint steering wheel module | Instrument Panel/Center Console Component Views | Component Connector End Views
HVAC Control Module | At the center of the instrument panel, above the radio | Instrument Panel/Center Console Component Views | Component Connector End Views
I/P Dimmer Switch | On the left side of the instrument panel, on knee bolster, next to the fog lamp switch | Instrument Panel/Center Console Component Views | Component Connector End Views
Ignition Coil 1 | At the top front side of the engine, above cylinder 1 | Powertrain Component Views | Component Connector End Views
Ignition Coil 2 | At the top front side of the engine, above cylinder 2 | Powertrain Component Views | Component Connector End Views
Ignition Coil 3 | At the top rear of the engine, above cylinder 3 | Powertrain Component Views | Component Connector End Views
Ignition Coil 4 | At the top rear of the engine, above cylinder 4 | Powertrain Component Views | Component Connector End Views
Ignition Switch | On the right side of the steering column | Instrument Panel/Center Console Component Views | Component Connector End Views
Inflatable Restraint Front End Sensor - Left | At the front of the vehicle, on the left frame rail attached to the back of the hinge bracket | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Inflatable Restraint Front End Sensor - Right | At the front of the vehicle, on the right frame rail attached to the back of the hinge bracket | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Inflatable Restraint I/P Module | Under the passenger side upper instrument panel pad, above the instrument panel compartment | Instrument Panel/Center Console Component Views | Component Connector End Views
Inflatable Restraint I/P Module Indicator | At the center of the instrument panel, to the right of the instrument panel cluster | Instrument Panel/Center Console Component Views | Component Connector End Views
Inflatable Restraint Passenger Presence System (PPS) Module | On the right side of the passenger compartment, under the passenger seat | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Located between the seats and under the center console | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Steering Wheel Module | At the top of the steering column, attached to the steering wheel | Instrument Panel/Center Console Component Views | Component Connector End Views
Inflatable Restraint Steering Wheel Module Coil | Near the top of the steering column, behind the steering wheel | Instrument Panel/Center Console Component Views | Component Connector End Views
Inline Fuse - Left Rear Lamps | In the instrument panel body harness approximately 60 mm from the breakout for connector 1 of the body control module | Passenger Compartment/Roof Component Views | Electrical Center Identification Views
Inline Fuse - Right Rear Lamps | In the instrument panel body harness approximately 60 mm from the breakout for connector 1 of the body control module | Passenger Compartment/Roof Component Views | Electrical Center Identification Views
Inside Rearview Mirror (ISRVM) | In the passenger compartment, attached to the center of the windshield | Instrument Panel/Center Console Component Views | Component Connector End Views
Instrument Panel Cluster (IPC) | At the left side of the instrument panel | Instrument Panel/Center Console Component Views | Component Connector End Views
Intake Air Pressure and Temperature Sensor | Left side of engine, near knock sensor 1 | Powertrain Component Views | Component Connector End Views
Knock Sensor (KS) 1 | Lower left front side of the engine | Powertrain Component Views | Component Connector End Views
Knock Sensor (KS) 2 | Lower left rear side of the engine | Powertrain Component Views | Component Connector End Views
License Lamp - Left | At the left center of the rear bumper | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
License Lamp - Right | At the right center of the rear bumper | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Manifold Absolute Pressure (MAP) Sensor | On the left side of the engine, near the throttle body, at intake port 3 | Powertrain Component Views | Component Connector End Views
Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor | At the front of the engine compartment, in the air intake duct near the throttle body | Powertrain Component Views | Component Connector End Views
Mode Actuator | In the passenger compartment, mounted on the left side of the HVAC module | Instrument Panel/Center Console Component Views | Component Connector End Views
Outside Air Temperature Sensor | On left front bumper fascia bracket | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Outside Rearview Mirror - Driver (D48) | At the front of the driver door | Door Component Views | Component Connector End Views
Outside Rearview Mirror - Passenger (D48) | At the front of the passenger door | Door Component Views | Component Connector End Views
Outside Rearview Mirror Switch (D48) | In the passenger compartment, on the driver door trim panel | Door Component Views | Component Connector End Views
Park Brake Switch | To the left of the park brake under the console | Instrument Panel/Center Console Component Views | Component Connector End Views
Park Lamp - Left Front | Part of the left headlamp assembly, at the left front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Park Lamp - Right Front | Part of the right headlamp assembly, at the right front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Radio | In the passenger compartment, at the center of the instrument panel | Instrument Panel/Center Console Component Views | Component Connector End Views
Radio Antenna | On the right rear quarter panel, just left of the rear compartment lid | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Rear Compartment Courtesy Lamp | In the rear compartment, on the right trim panel | Passenger Compartment/Roof Component Views | Component Connector End Views
Rear Compartment Lid Ajar Switch | At the front of the rear compartment, in the center, below the rear window | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Rear Compartment Lid Latch Release Actuator | At the front of the rear compartment, in the center, below the rear window | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Rear Compartment Lid Release Switch | In the instrument panel compartment, at the upper left corner | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Rear Window Defogger Grid | Mounted on the rear window | Passenger Compartment/Roof Component Views | Component Connector End Views
Recirculation Actuator | At the right side of the instrument panel, behind the instrument panel compartment | Instrument Panel/Center Console Component Views | Component Connector End Views
Remote Control Door Lock Receiver (RCDLR) | In the passenger compartment, behind the driver seat and to the right center of the rear support | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Adjuster Switch - Driver (AF2) | On the left side of the driver seat | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Pretensioner - Driver | In the left rear corner of the passenger compartment, part of the driver seat belt retractor | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Pretensioner - Passenger | In the right rear corner of the passenger compartment, part of the passenger seat belt retractor | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Switch - Driver | On the side of the driver seat, part of the seat belt buckle | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Switch - Passenger | On the side of the passenger seat, part of the seat belt buckle | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Front Vertical Motor - Driver (AF2) | Attached to the driver seat track | Passenger Compartment/Roof Component Views | Component Connector End Views
Speaker - Left Front | On the left door, at the lower front corner | Door Component Views | Component Connector End Views
Speaker - Left Rear | In the passenger compartment, in the left rear corner behind the driver seat | Passenger Compartment/Roof Component Views | Component Connector End Views
Speaker - Left Tweeter | At the left corner of the instrument panel, in the corner of the instrument panel trim pad | Instrument Panel/Center Console Component Views | Component Connector End Views
Speaker - Right Front | On the right door, at the lower front corner | Door Component Views | Component Connector End Views
Speaker - Right Rear | In the passenger compartment, in the right rear corner behind the passenger seat | Passenger Compartment/Roof Component Views | Component Connector End Views
Speaker - Right Tweeter | At the right corner of the instrument panel, in the corner of the instrument panel trim pad | Instrument Panel/Center Console Component Views | Component Connector End Views
Speaker - Subwoofer (UQ3) | In the rear compartment, at the right front corner | Passenger Compartment/Roof Component Views | Component Connector End Views
Starter Motor | Left side of engine, below the engine oil pressure switch | Powertrain Component Views | Component Connector End Views
Steering Angle Sensor | On steering column below bracket | Instrument Panel/Center Console Component Views | Component Connector End Views
Steering Wheel Control Switch - Left (K34) | At the top of the steering column, on the left side of the steering wheel | Instrument Panel/Center Console Component Views | Component Connector End Views
Steering Wheel Control Switch - Right (UK3) | At the top of the steering column, on the right side of the steering wheel | Instrument Panel/Center Console Component Views | Component Connector End Views
Tail/Stop Lamp - Left | Part of the left tail lamp assembly | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Tail/Stop Lamp - Right | Part of the right tail lamp assembly | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Theft Deterrent Module (TDM) | On the right side of the steering column, near the ignition lock cylinder | Instrument Panel/Center Console Component Views | Component Connector End Views
Throttle Body | On the left side of the engine compartment, above the exhaust manifold | Powertrain Component Views | Component Connector End Views
Traction Control Switch (TCS) | Center of the instrument panel, below the radio | Instrument Panel/Center Console Component Views | Component Connector End Views
Turbocharger Bypass Valve Solenoid | Top right of engine | Powertrain Component Views | Component Connector End Views
Turbocharger Wastegate Solenoid | Top right of engine | Powertrain Component Views | Component Connector End Views
Turn Signal Lamp - Left Front | Located in the left front corner of the front fascia | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Turn Signal Lamp - Left Rear | Part of the left tail lamp assembly | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Turn Signal Lamp - Right Front | Right front of the vehicle | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Turn Signal Lamp - Right Rear | Part of the right tail lamp assembly | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Turn Signal/Multifunction Switch | On the left side of the steering column | Instrument Panel/Center Console Component Views | Component Connector End Views
Turn Signal Repeater Lamp - Left | On the front of the left front wheelwell opening | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Turn Signal Repeater Lamp - Right | On the front of the right front wheelwell opening | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Vehicle Speed Sensor (VSS) | On the side of the transmission | Powertrain Component Views | Component Connector End Views
Wheel Speed Sensor (WSS) - Left Front | At the left front wheel, between the steering knuckle and brake rotor | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Wheel Speed Sensor (WSS) - Left Rear | At the left rear wheel, between the steering knuckle and brake rotor | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Wheel Speed Sensor (WSS) - Right Front | At the right front wheel, between the steering knuckle and brake rotor | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Wheel Speed Sensor (WSS) - Right Rear | At the right rear wheel, between the steering knuckle and brake rotor | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Window Motor - Driver (A31) | In the driver door, at the base of the window | Door Component Views | Component Connector End Views
Window Motor - Passenger (A31) | In the passenger door, at the base of the window | Door Component Views | Component Connector End Views
Window Switch - Driver (A31) | On the left door trim panel | Door Component Views | Component Connector End Views
Window Switch - Passenger (A31) | On the right door trim panel | Door Component Views | Component Connector End Views
Windshield Washer Fluid Pump | Behind the left front wheel well, mounted at the bottom of the washer fluid reservoir | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Windshield Wiper Motor | On the left side of the cowl, mounted to the wiper transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Windshield Wiper/Washer Switch | On the right side of the steering column, on the right stalk | Instrument Panel/Center Console Component Views | Component Connector End Views
Yaw and Lateral Accelerometer Sensor | Attached to the floor panel on the right side of the floor tunnel panel | Passenger Compartment/Roof Component Views | Component Connector End Views
X100 (40 Cavities) | Instrument panel body harness to the engine harness, right rear of the engine compartment, below the fuse block underhood | Harness Routing Views | Inline Harness Connector End Views
X102 (4 Cavities) | Forward lamp harness to the right fog turn signal harness, front right of the engine compartment | Harness Routing Views | Inline Harness Connector End Views
X103 (4 Cavities) | Forward lamp harness to the left fog turn harness, front left of the engine compartment | Harness Routing Views | Inline Harness Connector End Views
X110 (4 Cavities) | Forward lamp harness to left headlamp assembly harness | Harness Routing Views | Inline Harness Connector End Views
X111 (4 Cavities) | Forward lamp harness to right headlamp assembly harness | Harness Routing Views | Inline Harness Connector End Views
X120 (16 Cavities) | Instrument panel body harness to the forward lamp harness, right rear of the engine compartment below fuse block underhood | Harness Routing Views | Inline Harness Connector End Views
X122 (2 Cavities) | Instrument panel body harness to the forward lamp harness, under the underhood fuse block, approximately 30 cm (11.8 in) from X100 | Harness Routing Views | Inline Harness Connector End Views
X162 (12 Cavities) | Engine harness to the fuel injector harness, approximately 16.5 cm (6.5 in) from the main breakout, near knock sensor 1 | Harness Routing Views | Inline Harness Connector End Views
X208 (4 Cavities) | Passenger air bag harness to instrument panel body harness, behind the instrument panel, driver side, near the rear compartment lid release switch | Harness Routing Views | Inline Harness Connector End Views
X216 (8 Cavities) | Instrument panel body harness to the HVAC harness, right side of instrument panel, behind glove box | Harness Routing Views | Inline Harness Connector End Views
X218 (12 Cavities) | Instrument panel body harness to the HVAC harness, right side of instrument panel, behind glove box | Harness Routing Views | Inline Harness Connector End Views
X316 (8 Cavities) | Instrument panel body harness to the right front seat harness, under the right front seat approximately 168 cm (66 in) from the radio antenna breakout | Harness Routing Views | Inline Harness Connector End Views
X317 (4 Cavities) (AF2) | Instrument panel body harness to the driver seat harness, under the driver seat | Harness Routing Views | Inline Harness Connector End Views
X317 (3 Cavities) (without AF2) | Instrument panel body harness to the driver seat harness, under the driver seat | Harness Routing Views | Inline Harness Connector End Views
X400 (4 Cavities) | Instrument panel body harness to the rear lamp harness, in front of the right rear tail lamp | Harness Routing Views | Inline Harness Connector End Views
X405 (6 Cavities) | Rear chassis harness to the left rear tail lamp assembly harness, on the left tail lamp assembly | Harness Routing Views | Inline Harness Connector End Views
X406 (8 Cavities) | Instrument panel body harness to the rear chassis harness, approximately 16 cm (6.3 in) from the X408 breakout | Harness Routing Views | Inline Harness Connector End Views
X407 (6 Cavities) | Rear chassis harness to the right rear tail lamp assembly harness, on the right tail lamp assembly | Harness Routing Views | Inline Harness Connector End Views
X408 (8 Cavities) | Rear chassis harness to the instrument panel body harness, approximately 15 cm (5.9 in) from the breakout for X410 | Harness Routing Views | Inline Harness Connector End Views
X409 (1 Cavity) | Instrument panel body harness to rear chassis harness, approximately 12 cm (4.7 in) from the X410 breakout | Harness Routing Views | Inline Harness Connector End Views
X410 (6 Cavities) | Instrument panel body harness to the rear lamp jumper harness, at the center of rear fascia in rear compartment | Harness Routing Views | Inline Harness Connector End Views
X500 (10 Cavities) | Instrument panel body harness to the left door harness, under hood at left hood hinge | Harness Routing Views | Inline Harness Connector End Views
X501 (8 Cavities) | Instrument panel body harness to the left door harness, under hood at left hood hinge | Harness Routing Views | Inline Harness Connector End Views
X600 (16 Cavities) | Instrument panel body harness to the right door harness, under hood at right hood hinge | Harness Routing Views | Inline Harness Connector End Views
G101 | At the left front corner of the engine compartment, mounted on the frame rail, rearward of G105 | Ground Views | --
G102 | At the right front corner of the engine compartment, mounted on the frame rail | Ground Views | --
G103 | On the engine, at the lower right rear corner | Ground Views | --
G104 | On the right front corner of the engine | Ground Views | --
G105 | At the left front corner of the engine compartment, mounted on the frame rail, forward of G101 | Ground Views | --
G106 | In the engine compartment, under the underhood fuse block, mounted on the outside of the frame rail | Ground Views | --
G300 | In the passenger compartment, under the center console | Ground Views | --
G301 | In the passenger compartment, in the corner behind the driver seat, on the B-pillar | Ground Views | --
G302 | In the passenger compartment, in the corner behind the passenger seat, on the B-pillar | Ground Views | --
G303 | In the passenger compartment, mounted on the rear support behind the driver seat | Ground Views | --
G304 | In the passenger compartment, behind the passenger seat | Ground Views | --
G400 | At the rear of the vehicle, on the right rear frame rail, above the right rear wheel | Ground Views | --
G402 | At the rear of the vehicle, on the outside of the right rear frame rail | Ground Views | --
J100 | In the forward lamp harness, approximately 40.5 cm (16 in) from the horn breakout towards the outside air temperature sensor breakout (CKT 9) | Harness Routing Views | --
J101 | In the forward lamp harness, approximately 10 cm (3.9 in) from the electrical brake control module (EBCM) (CKT 542) | Harness Routing Views | --
J102 | In the engine harness, approximately 15 cm (5.9 in) from the brake fluid level switch towards the engine control module (ECM) breakout (CKT 2700) | Harness Routing Views | --
J103 | In the forward lamp harness, approximately 10 cm (3.9 in) from the outside air temperature sensor breakout towards G105 and G101 (CKT 150) | Harness Routing Views | --
J104 | In the engine harness, approximately 12 cm (4.7 in) from the generator breakout towards the EVAP canister purge solenoid (CKT 250) | Harness Routing Views | --
J105 | In the forward lamp harness (CKT 250) | Harness Routing Views | --
J107 | In the engine harness, approximately 3 cm (1.2 in) from the heated oxygen sensor 1 breakout towards ignition coil 3 (CKT 450) | Harness Routing Views | --
J108 | In the engine harness, approximately 5 cm (2.0 in) from the brake fluid level switch breakout towards the engine control module (ECM) (CKT 451) | Harness Routing Views | --
J109 | In the forward lamp harness (CKT 350) | Harness Routing Views | --
J110 | In the engine harness, approximately 10 cm (3.9 in) from the brake fluid level switch breakout towards the engine control module (ECM) (CKT 5514) | Harness Routing Views | --
J115 | In the forward lamp harness, approximately 8 cm (3.1 in) from G102 breakout towards the cooling fan breakout (CKT 2234) | Harness Routing Views | --
J116 | In the engine harness, approximately 13.5 cm (5.3 in) from X100 towards G104 breakout (CKT 24) | Harness Routing Views | --
J117 | In the engine harness, approximately 11.5 cm (4.5 in) from the ignition coil 1 breakout towards X100 (CKT 5292) | Harness Routing Views | --
J121 | In the engine harness, approximately 4.5 cm (1.7 in) from G104 breakout towards X100 (CKT 5293) | Harness Routing Views | --
J123 | In the engine harness, approximately 3 cm (1.2 in) from ignition coil 3 breakout towards ignition coil 4 breakout (CKT 2130) | Harness Routing Views | --
J124 | In the engine harness, approximately 3 cm (1.2 in) from ignition coil 3 breakout towards ignition coil 2 breakout (CKT 2129) | Harness Routing Views | --
J126 | In the engine harness, approximately 4.5 cm (1.8 in) from G104 breakout towards the intake air pressure and temperature sensor breakout (CKT 705) | Harness Routing Views | --
J128 | In the forward lamp harness, approximately 25.5 cm (10 in) from the underhood fuse block (CKT 833) | Harness Routing Views | --
J129 | In the forward lamp harness, approximately 28 cm (11 in) from the underhood fuse block (CKT 872) | Harness Routing Views | --
J130 | In the forward lamp harness, approximately 21 cm (8.3 in) from the left front wheel speed sensor breakout, towards the electronic brake control module (CKT 830) | Harness Routing Views | --
J131 | In the forward lamp harness, approximately 15 cm (5.9 in) from the electronic brake control module (CKT 873) | Harness Routing Views | --
J134 | In the instrument panel body harness, approximately 29.5 cm (11.6 in) from the underhood fuse block X2 connector breakout towards the underhood fuse block X4 connector (CKT 20) | Harness Routing Views | --
J137 | In the engine harness, approximately 4 cm (1.6 in) from the engine coolant level switch breakout towards the windshield washer fluid pump (CKT 5290) | Harness Routing Views | --
J140 | In the engine harness, approximately 5 cm (2.0 in) from ignition coil 4 breakout towards G103 (CKT 552) | Harness Routing Views | --
J141 | In the engine harness, approximately 15 cm (5.9 in) from the windshield washer fluid pump towards the brake fluid switch (CKT 407) | Harness Routing Views | --
J142 | In the engine harness, approximately 7 cm (2.8 in) from the manifold absolute pressure sensor breakout towards the generator breakout (CKT 597) | Harness Routing Views | --
J145 | In the forward lamp harness, 7 cm (2.8 in) from the outside air temperature sensor breakout (CKT 14) | Harness Routing Views | --
J146 | In the forward lamp harness, 27 cm (10.8 in) from the X120 breakout (CKT 15) | Harness Routing Views | --
J147 | In the forward lamp harness, 32.5 cm (13.0 in) from the X120 breakout (CKT 29) | Harness Routing Views | --
J200 | In the instrument panel body harness, approximately 33 cm (13 in) from the rear compartment lamp breakout towards the rear defogger grid (CKT 9) | Harness Routing Views | --
J201 | In the instrument panel body harness, approximately 40 cm (15.7 in) from the underhood fuse block (CKT 5291) | Harness Routing Views | --
J203 | In the instrument panel body harness, approximately 10 cm (3.9 in) from the HVAC module breakout, towards the steering column (CKT 1540) | Harness Routing Views | --
J204 | In the instrument panel body harness, approximately 5.5 cm (2.2 in) from the body control module X1 connector breakout towards the JX200 breakout (CKT 1970) | Harness Routing Views | --
J205 | In the instrument panel body harness, approximately 8 cm (3.1 in) from G300 breakout towards the radio antenna breakout (CKT 1339) | Harness Routing Views | --
J208 | In the instrument panel body harness, approximately 8 cm (3.1 in) from the instrument panel cluster breakout, towards the ambient light sensor (CKT 550) | Harness Routing Views | --
J209 | In the instrument panel body harness, approximately 4 cm (1.6 in) from the hazard warning switch breakout towards the accessory power outlet breakout (CKT 8) | Harness Routing Views | --
J211 (UW5) | In the instrument panel body harness (CKT 117) | Harness Routing Views | --
J212 (UW5) | In the instrument panel body harness (CKT 200) | Harness Routing Views | --
J213 | In the instrument panel body harness (CKT 240) | Harness Routing Views | --
J214 | In the instrument panel body harness, approximately 74 cm (29 in) from G301 breakout towards the driver door grommet (CKT 56) | Harness Routing Views | --
J216 | In the instrument panel body harness, approximately 7 cm (2.8 in) from the accelerator pedal position sensor breakout, towards the steering wheel (CKT 4) | Harness Routing Views | --
J219 | In the instrument panel body harness, approximately 11.5 cm (4.5 in) from the data link connector (CKT 2501) | Harness Routing Views | --
J220 | In the instrument panel body harness, approximately 10 cm (3.9 in) from the data link connector (CKT 2500) | Harness Routing Views | --
J221 (UW5) | In the instrument panel body harness (CKT 118) | Harness Routing Views | --
J222 (UW5) | In the instrument panel body harness (CKT 201) | Harness Routing Views | --
J225 | In the HVAC harness (CKT 141) | Harness Routing Views | --
J226 | In the instrument panel body harness, approximately 4.5 cm (1.8 in) from the accessory power outlet towards the passenger air bag (CKT 550) | Harness Routing Views | --
J231 | In the HVAC harness (CKT 1791) | Harness Routing Views | --
J232 | In the HVAC harness (CKT 2273) | Harness Routing Views | --
J233 | In the HVAC harness (CKT 1688) | Harness Routing Views | --
J234 | In the HVAC harness (CKT 1647) | Harness Routing Views | --
J235 | In the steering wheel harness (CKT 1150) | Harness Routing Views | --
J300 | In the instrument panel body harness, approximately 31 cm (12.2 in) from G300 breakout towards the radio antenna (CKT 651) | Harness Routing Views | --
J301 | In the instrument panel body harness (CKT 5057) | Harness Routing Views | --
J302 (AF2) | In the driver seat harness, approximately 5 cm (2 in) from the seat vertical motor breakout, towards the seat adjuster switch (CKT 550) | Harness Routing Views | --
J303 | In the instrument panel body harness, approximately 10 cm (3.9 in) from the yaw and lateral accelerometer sensor breakout, towards the subwoofer (CKT 2087) | Harness Routing Views | --
J304 | In the instrument panel body harness, approximately 18 cm (7.1 in) from the yaw and lateral accelerometer sensor breakout, towards the subwoofer (CKT 2088) | Harness Routing Views | --
J311 | In the instrument panel body harness (CKT 850) | Harness Routing Views | --
J318 | In the instrument panel Body harness (CKT 1339) | Harness Routing Views | --
J400 | In the instrument panel body harness (CKT 850) | Harness Routing Views | --
J401 | In the rear chassis harness, approximately 7.5 cm (3 in) from X408 breakout (CKT 750) | Harness Routing Views | --
J402 | In the right tail lamp harness (CKT 750) | Harness Routing Views | --
J403 | In the instrument panel body harness, approximately 16.5 cm (6.5 in) from X400 (CKT 750) | Harness Routing Views | --
J405 | In the left tail lamp harness, approximately 5 cm (2 in) from X405 (CKT 2759) | Harness Routing Views | --
J406 | In the left tail lamp harness, approximately 5 cm (2 in) from X405 (CKT 9) | Harness Routing Views | --
J407 | In the right tail lamp harness, approximately 5 cm (2 in) from X406 (CKT 9) | Harness Routing Views | --
J408 | In the left tail lamp harness, approximately 5 cm (2 in) from X405 (CKT 18) | Harness Routing Views | --
J409 | In the right tail lamp harness, approximately 5 cm (2 in) from X406 (CKT 19) | Harness Routing Views | --
J410 | In the rear chassis harness, approximately 82 cm (32 in) from the left rear wheel speed sensor towards the left tail lamp assembly (CKT 750) | Harness Routing Views | --
J416 | In the rear lamp harness, approximately 17.5 cm (6.8 in) from X400 towards the CHMSL breakout (CKT 750) | Harness Routing Views | --
J421 | In the rear chassis harness, approximately 18.5 cm (7.3 in) from the right tail lamp breakout towards the left tail lamp (CKT 9) | Harness Routing Views | --
J422 | In the rear chassis harness, near the X406 breakout (CKT 20) | Harness Routing Views | --
J500 | In the left front door harness (CKT 550) | Harness Routing Views | --
J501 | In the left front door harness, approximately 32 cm (12.6 in) from the outside rearview mirror switch towards the mirror (CKT 8) | Harness Routing Views | --
J600 | In the right front door harness, approximately 8 cm (3.1 in) from the door grommet towards the passenger window switch (CKT 550) | Harness Routing Views | --
JX200 | In the passenger compartment, in the right front footwell area next to the body control module (BCM) | Harness Routing Views | Splice Pack Connector End Views