For 1990-2009 cars

Connector 1: | Ignition Switch

### Ignition Switch

#### Connector Part Information

- OEM: 1L-AG5-6S-S3C1
- Description: 6-Way F 1L - AG5 Series (GN)

#### Ignition Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 RD/WH | 1040 | Battery Positive Voltage
3 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
4 | 0.35 BN | 4 | Accessory Voltage
5 | 0.35 WH | 1390 | Off/Run/Crank Voltage
6 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal