For 1990-2009 cars

Connector 1: | Accelerator Pedal Position (APP) Sensor
Connector 2: | Camshaft Position (CMP) Actuator Solenoid - Exhaust
Connector 3: | Camshaft Position (CMP) Actuator Solenoid - Intake
Connector 4: | Camshaft Position (CMP) Sensor - Exhaust
Connector 5: | Camshaft Position (CMP) Sensor - Intake
Connector 6: | Crankshaft Position (CKP) Sensor
Connector 7: | Engine Coolant Temperature (ECT) Sensor
Connector 8: | Evaporative Emission (EVAP) Canister Purge Solenoid
Connector 9: | Evaporative Emission (EVAP) Canister Vent Solenoid
Connector 10: | Fuel Injector 1
Connector 11: | Fuel Injector 2
Connector 12: | Fuel Injector 3
Connector 13: | Fuel Injector 4
Connector 14: | Fuel Rail Pressure (FRP) Sensor
Connector 15: | Fuel Pump and Sender Assembly
Connector 16: | Fuel Tank Pressure (FTP) Sensor
Connector 17: | Heated Oxygen Sensor (HO2S) 1
Connector 18: | Heated Oxygen Sensor (HO2S) 2
Connector 19: | High Pressure Fuel Pump
Connector 20: | Ignition Coil 1
Connector 21: | Ignition Coil 2
Connector 22: | Ignition Coil 3
Connector 23: | Ignition Coil 4
Connector 24: | Intake Air Pressure and Temperature Sensor
Connector 25: | Knock Sensor (KS) - 1
Connector 26: | Knock Sensor (KS) - 2
Connector 27: | Manifold Absolute Pressure (MAP) Sensor
Connector 28: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 29: | Throttle Body
Connector 30: | Turbo Bypass Valve Control Solenoid
Connector 31: | Turbocharger Wastegate Solenoid

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15326829
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | Low Reference
B | 0.35 L-BU | 1162 | TP Sensor 2 Signal
C | 0.35 TN | 1274 | 5-Volt Reference 3
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | TP Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference 2

### Camshaft Position (CMP) Actuator Solenoid - Exhaust

#### Connector Part Information

- OEM: 15336004
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Actuator Solenoid - Exhaust

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)
B | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid Control

### Camshaft Position (CMP) Actuator Solenoid - Intake

#### Connector Part Information

- OEM: 15335987
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Actuator Solenoid - Intake

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)
B | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid Control

### Camshaft Position (CMP) Sensor - Exhaust

#### Connector Part Information

- OEM: 15326808
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Sensor - Exhaust

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 GY | 705 | 5-Volt Reference 2
B | 0.5 TN | 552 | Low Reference
C | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor Signal 1

### Camshaft Position (CMP) Sensor - Intake

#### Connector Part Information

- OEM: 15326808
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Sensor - Intake

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 GY | 705 | 5-Volt Reference 2
B | 0.5 TN | 552 | Low Reference
C | 0.5 OG | 5275 | Camshaft Position Intake Sensor Signal

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 31403-3700 (Delphi # 13521040)
- Description: 3-Way F MX64 Series, Sealed (BK)

#### Crankshaft Position (CKP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.35 GY | 605 | 5-Volt Reference 3
2 | 0.35 TN | 452 | Low Reference
3 | 0.35 YE | 573 | Crankshaft Position Sensor Signal

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 15449028
- Description: 2-Way F GT 150 Sealed (BK)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 TN | 2761 | Low Reference
B | 0.5 YE | 410 | ECT Sensor Signal

### Evaporative Emission (EVAP) Canister Purge Solenoid

#### Connector Part Information

- OEM: 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Purge Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage
B | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid

#### Connector Part Information

- OEM: 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 140 | Battery Positive Voltage
B | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control

### Fuel Injector 1

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.0 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 1.0 TN | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1

### Fuel Injector 2

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.0 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
2 | 1.0 TN | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2

### Fuel Injector 3

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.0 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
2 | 1.0 TN | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3

### Fuel Injector 4

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.0 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
2 | 1.0 TN | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4

### Fuel Rail Pressure (FRP) Sensor

#### Connector Part Information

- OEM: 1 928 403 966
- Description: 3-Way F 2.8 Series Sealed (BK)

#### Fuel Rail Pressure (FRP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GY | 808 | Sensor Low Reference
2 | 0.5 GY | 2918 | Fuel Rail Pressure Sensor Signal
3 | 0.5 GY | 598 | 5-Volt Reference 1

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 15326631
- Description: 4-Way F GT 280 Series Sealed (BK)

#### Fuel Pump and Sender Assembly

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1.0 BK | 750 | Ground
B | 0.5 PU | 1589 | Fuel Level Sensor Signal
C | 0.5 TN | 2759 | Low Reference
D | 1.0 GY | 120 | Fuel Pump Supply Voltage

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 TN | 2759 | Low Reference
B | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
C | 0.5 GY | 2709 | 5-Volt Reference 1

### Heated Oxygen Sensor (HO2S) 1

#### Connector Part Information

- OEM: 1 928 404 900
- Description: 6-Way F Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 WH | 5279 | Heated Oxygen Sensor Pump Current - Sensor 1
2 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal - Sensor 1
3 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control - Sensor 1
4 | 0.5 PK/BK | 5291 | Ignition 1 Voltage
5 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current - Sensor 1
6 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal - Sensor 1

### Heated Oxygen Sensor (HO2S) 2

#### Connector Part Information

- OEM: 15326423
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal - Sensor 2
B | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal - Sensor 2
C | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control - Sensor 2
D | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### High Pressure Fuel Pump

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### High Pressure Fuel Pump

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.0 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
2 | 1.0 YE | 7301 | High Pressure Fuel Pump Actuator High Control

### Ignition Coil 1

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN | 2129 | Low Reference
3 | 0.35 PU | 2121 | IC 1 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 2

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN/WH | 2130 | Low Reference
3 | 0.35 OG/WH | 2122 | IC 2 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 3

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN | 2129 | Low Reference
3 | 0.35 L-BU | 2123 | IC 3 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 4

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN/WH | 2130 | Low Reference
3 | 0.35 D-GN/WH | 2124 | IC 4 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Intake Air Pressure and Temperature Sensor

#### Connector Part Information

- OEM: 12162187
- Description: 4-Way F Metri-Pack 150.2 Series Sealed, Pull to Seat (BK)

#### Intake Air Pressure and Temperature Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 TN | 407 | Low Reference
B | 0.5 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
C | 0.5 GY | 597 | 5-Volt Reference 1
D | 0.5 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal

### Knock Sensor (KS) - 1

#### Connector Part Information

- OEM: 12077900
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Knock Sensor (KS) - 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 D-BU | 496 | KS 1 Signal
B | 0.5 GY | 1716 | KS 1 Signal

### Knock Sensor (KS) - 2

#### Connector Part Information

- OEM: 12077900
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Knock Sensor (KS) - 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1876 | KS 2 Signal
B | 0.5 GY | 2303 | KS 2 Signal

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: 184032-1
- Description: 3-Way F SSC Sealed Series (BK)

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GY | 597 | 5-Volt Reference 1
2 | 0.5 TN | 407 | Low Reference
3 | 0.5 L-GN | 432 | MAP Sensor Signal

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 15326822
- Description: 5-Way F GT 150 Series Sealed (BK)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.35 YE | 492 | MAF Sensor Signal
B | 0.35 BK/WH | 451 | Ground
C | 0.35 PK/BK | 5291 | Ignition 1 Voltage
D | 0.35 TN | 2760 | Low Reference
E | 0.35 L-BU | 6289 | Induction Air Temperature Sensor Signal

### Throttle Body

#### Connector Part Information

- OEM: 15355297
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Throttle Body

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 BN | 582 | TAC Motor Control - 2
B | 0.8 YE | 581 | TAC Motor Control - 1
C | 0.5 TN | 2752 | Low Reference
D | 0.5 D-GN | 485 | TP Sensor 1 Signal
E | 0.5 GY | 2701 | 5-Volt Reference 3
F | 0.5 PU | 486 | TP Sensor 2 Signal

### Turbo Bypass Valve Control Solenoid

#### Connector Part Information

- OEM: 1 928 402 571
- Description: 2-Way F Sealed (BK)

#### Turbo Bypass Valve Control Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 6391 | Turbo Bypass Valve Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turbocharger Wastegate Solenoid

#### Connector Part Information

- OEM: 1 928 402 571
- Description: 2-Way F Sealed (BK)

#### Turbocharger Wastegate Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE | 258 | Wastegate Solenoid Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)