For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the General Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Verify the vehicle leans or sways in corners. Does the vehicle operate normally? | System OK | Go to Step 3
3 | Inspect the following components for wear or damage:

• | Rear Coil Springs

• | Front Coil Springs

Are the components worn or damaged?

Go to Step 5

Go to Step 4

4 |

1. Inspect the stabilizer shaft link for wear or damage.
2. Repair as necessary.

Did you find and correct the condition?

Go to Step 6

Go to Step 2

5 | Replace the springs as necessary. Did you complete the repair? | Go to Step 6 | --
6 | Operate the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3