For 1990-2009 cars

Connector 1: | Electronic Brake Control Module (EBCM)
Connector 2: | Steering Angle Sensor (JL4)
Connector 3: | Traction Control Switch (NW9/JL4)
Connector 4: | Wheel Speed Sensor (WSS) - Left Front
Connector 5: | Wheel Speed Sensor (WSS) - Left Rear
Connector 6: | Wheel Speed Sensor (WSS) - Right Front
Connector 7: | Wheel Speed Sensor (WSS) - Right Rear
Connector 8: | Yaw and Lateral Accelerometer Sensor (JL4)

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: 1355628-2
- Description: 47-Way F MK25/60 Series (BK)

#### Electronic Brake Control Module (EBCM)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 3.0 RD/BK | 542 | Low Reference
2-7 | -- | -- | Not Used
8 | 0.5 PK | 1439 | Ignition 1 Voltage
9-10 | -- | -- | Not Used
11 | 0.5 TN/BK | 2500 | High Speed Serial Data Bus (+)
12 | 0.5 TN/BK | 2500 | High Speed Serial Data Bus (+)
13 | 0.5 TN | 2501 | High Speed Serial Data Bus (-)
14 | 0.5 TN | 2501 | High Speed Serial Data Bus (-)
15 | -- | -- | Not Used
16 | 3.0 BK | 350 | Ground
17 | -- | -- | Not Used
18 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
19 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
20-21 | -- | -- | Not Used
22 | 0.5 D-GN | 2087 | 12-Volt Reference
23-28 | -- | -- | Not Used
29 | 0.5 L-BU | 2088 | Low Reference
30-31 | -- | -- | Not Used
32 | 2.0 RD/WH | 540 | Battery Positive Voltage
33 | 0.5 TN | 833 | Low Reference
34 | 0.5 D-GN | 872 | Wheel Speed Sensor Signal (WSS) - Right Front
35 | -- | -- | Not Used
36 | 0.5 TN | 884 | Wheel Speed Sensor Signal (WSS) - Left Rear
37 | 0.5 OG | 885 | Low Reference
38-41 | -- | -- | Not Used
42 | 0.5 WH | 883 | Low Reference
43 | 0.5 BN | 882 | Wheel Speed Sensor Signal (WSS) - Right Rear
44 | -- | -- | Not Used
45 | 0.5 L-BU | 830 | Wheel Speed Sensor Signal (WSS) - Left Front
46 | 0.5 YE | 873 | Low Reference
47 | -- | -- | Not Used

### Steering Angle Sensor (JL4)

#### Connector Part Information

- OEM: 1488752-1
- Description: 6-Way F 064 GET Series (BK)

#### Steering Angle Sensor (JL4)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 2087 | 12-Volt Reference
2 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
3 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
4 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
5 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
6 | 0.5 L-BU | 2088 | Low Reference

### Traction Control Switch (NW9/JL4)

#### Connector Part Information

- OEM: 12047785
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Traction Control Switch (NW9/JL4)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.35 BK | 550 | Ground
B | -- | -- | Not Used
C | 0.35 L-BU | 1788 | Traction Control Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

- OEM: 1-928-403-698
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Left Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.8 L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | 0.8 YE | 873 | Low Reference

### Wheel Speed Sensor (WSS) - Left Rear

#### Connector Part Information

- OEM: 1-928-403-698
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Left Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.8 TN | 884 | Left Rear Wheel Speed Sensor Signal
2 | 0.8 OG | 885 | Low Reference

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

- OEM: 1-928-403-698
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Right Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.8 D-GN | 872 | Right Front Wheel Speed Sensor Signal
2 | 0.8 TN | 833 | Low Reference

### Wheel Speed Sensor (WSS) - Right Rear

#### Connector Part Information

- OEM: 1-928-403-698
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Right Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal
2 | 0.8 WH | 883 | Low Reference

### Yaw and Lateral Accelerometer Sensor (JL4)

#### Connector Part Information

- OEM: 2-967616-1
- Description: 6-Way F MQS Socket Series, Sealed (BK)

#### Yaw and Lateral Accelerometer Sensor (JL4)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
2 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
3 | 0.5 D-GN | 2087 | 12-Volt Reference
4 | -- | -- | Not Used
5 | 0.5 L-BU | 2088 | Low Reference
6 | -- | -- | Not Used