For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Back Up and Rear Fog Lamp Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Back Up and Rear Fog Lamp Assembly Caution: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Disconnect the electrical connectors to the back up lamps and rear fog lamp.
2. Transfer the bulb sockets with bulbs as needed.