For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle's RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
AF2 | Adjuster - Seat, Power, 2 Way, Vertical, Driver
AL0 | Sensor Indicator - Inflatable Restraint, Front Passenger/Child Presence Detector
AU3 | Lock Control - Side Door, Electric
AZ5 | Covering Headliner - Convertible Top Trim
A31 | Window - Power Operated, All Doors
A50 | Seat - Front Bucket
B32 | Covering Front - Floor Mats, Auxiliary
B70 | Plate - Door Sill Cover
CE7 | Certification - Emission, Exported Vehicle
C4E | Country - Europe
C60 | HVAC System - Air Conditioner Front, Manual Controls
D48 | Mirror Outside - LH and RH, Remote Control, Electric, Color
EXP | Export
FE3 | Suspension System - Sport
GT4 | Axle Rear - 3.73 Ratio
G80 | Axle Positracton - Limited Slip
IPB | Trim - Interior Design (PB)
IP2 | Trim - Interior Trim (P2)
JL4 | Control - Active Brake
JL9 | Brake System - Power, Front and Rear Disc, Antilock, Front and Rear Wheel
KG9 | Generator - 140 Amp
K34 | Cruise Control - Automatic, Electronic
LNF | Engine - Gas, 4 Cyl, 2.0L, DI, Alum, DOHC, Turbo, GM
MA5 | Transmission - Manual 5 Spd, Aisin, 82 mm, 3.753 1st, 0.729 5th
MM5 | Merchandised Transmission - Manual 5 Spd Provisions
M82 | Transmission - Automatic 5 Spd, HMD, 5L40-E, Electronic
NT4 | Emission System - EEC 05
N34 | Steering Wheel - Leather, 3 Spokes
N87 | Wheel - 18 x 8, Aluminum
QSL | Tire All - P245/45R18-96W BW TL HW4
T96 | Lamp - Fog, Front
UK3 | Control - Steering Wheel, Accessory
UQ3 | Speaker System - Enhanced Audio
US6 | Antenna - Fixed, Painted, Radio
US8 | Radio - AM/FM Stereo, Seek/Scan, CD, Auto Tone, Clock, ETR, MP3, RDS
US9 | Radio - AM/FM Stereo, Seek/Scan, RDS, Multiple Compact Disc, Auto Tone Control, Clock, ETR, MP3
UW5 | Speaker System - 6, Base
U19 | Speedometer - Instrument, Kilo and Miles, Kilo Odometer
U68 | Display - Driver Information Center (DIC)
VH5 | Plate - Vehicle Identification
VK3 | License Plate Front - Front Mounting Package
VY7 | Knob - Transmission Control Lever, Leather
WIL | Plant Code - Wilmington, Delaware, USA
19B | Trim Combination - Cloth, Ebony (B) (00)
19T | Top Color - Convertible, Black
25U | Primary Color - Exterior, Dark Ming Blue (02)
34U | Primary Color - Exterior, Yellow (02) (WA 9414)
38U | Primary Color - Exterior, Emerald Jewel Met (05)
41U | Primary Color - Exterior, Black (02)
42U | Primary Color - Exterior, DK Tarnished Silver Met (04)
67U | Primary Color - Exterior, Light Tarnished Silver Met (04)
50U | Primary Color - Exterior, Olympic White (02)
72U | Primary Color - Exterior, Bluestone Met (04)
74U | Primary Color - Exterior, Victory Red (02)
021 | Interior Trim - Cobalt Red (04)
025 | Trim Combination - Leather, Cobalt Red (2) (7)
191 | Interior Trim - Ebony (1) (00)
192 | Trim Combination - Leather, Ebony (2) (00)