For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
Important: Do not clear any DTCs unless instructed to do so by a diagnostic procedure Important: If any DTCs are Powertrain related DTCs, select Capture Info in order to store the DTC information with the scan tool. Diagnose any current DTCs in the following order:

1. DTCs that begin with a U
2. Any of the following: B1000, B1001, B1004, B1009, B1019, C0550, C0551, C0561, C0569, P0601, P0602, P0603, P0604, P0606, P062B, P167D, P2107, or P2610
3. Any of the following: B1325, B1370, B1424, C0899, C0900, P0560, P0562, or P0563
4. Component level DTCs
5. System level DTCs
6. Any remaining DTCs

B0012 | Driver Frontal Deployment Loop Stage 1 Circuit | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 Circuit | SDM | DTC B0012 or B0013
B0015 | Driver Pretensioner Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0022 | Passenger Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0052 | Deployment Commanded | SDM | DTC B0052 or B0053
B0053 | Deployment Commanded with Loop DTCs Present | SDM | DTC B0052 or B0053
B0081 | Passenger Presence System | SDM | DTC B0081
B0083 | Front End Sensor 1 | SDM | DTC B0083 or B0084
B0084 | Front End Sensor 2 | SDM | DTC B0083 or B0084
B0283 | Electric Rear Defrost Circuit | BCM | DTC B0283
B1000 | Electronic Control Unit Performance | BCM, IPC, Radio, RCDLR, SDM, TDM, VCIM | DTC B1000
B1001 | Option Configuration Error | BCM | DTC B1001
SDM | DTC B1001
B1004 | Keep Alive Memory (KAM) Reset | BCM | DTC B1004
B1009 | EEPROM Checksum Mismatch | BCM | DTC B1009
B1019 | System Configuration Error | SDM | DTC B1019
B1025 | Left Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Right Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Left Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Right Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1287 | External Amp Control | Radio | DTC B1287
B1325 | Device Power 1 Circuit | BCM, IPC, Radio, SDM | DTC B1325
B1370 | Device Ignition 1 Circuit | BCM | DTC B1370
SDM | DTC B1370
B1380 | Device Ignition ACCESSORY Circuit | BCM | DTC B1380
B1424 | Device 1 Voltage Low | TDM | DTC B1424
B1441 | Device Ignition OFF, RUN and CRANK Circuit | BCM | DTC B1441
B1480 | Battery Rundown Protection Circuit | BCM | DTC B1480
B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2555 | Passenger Compartment Lamp Control Circuit | BCM | DTC B2555
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2625 | Display Dimming Pulse Width Modulation (PWM) Output Circuit | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2750 | Horn Relay Control Circuit | BCM | DTC B2750
B2961 | Key In Ignition Circuit | BCM | DTC B2961
B3031 | Security System Controller In Learn Mode | TDM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | TDM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | TDM | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | RCDLR | DTC B3105
B3109 | Keyless Entry Transmitter 1 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3110 | Keyless Entry Transmitter 2 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3111 | Keyless Entry Transmitter 3 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3112 | Keyless Entry Transmitter 4 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3265 | Trunk Relay Output Circuit | BCM | DTC B3265
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3903 | Stop Lamp Relay Circuit | BCM | DTC B3903
B3935 | Transponder Authentication Error | TDM | DTC B3935
B3948 | Left Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3949 | Right Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3950 | Left Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3951 | Right Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3976 | Unconfigured Transponder/Vehicle Configuration Not Programmed | TDM | DTC B3976
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | Antilock Brake System (ABS) Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Brake System (ABS) Brake Switch/Sensor Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0196 | Yaw Rate Circuit | EBCM | DTC C0196
C0201 | Antilock Brake System (ABS) Enable Relay Contact Circuit | EBCM | DTC C0201
C0252 | Steering Wheel Position Sensor | EBCM | DTC C0252
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0277 | Brake Pedal Position Sensor Circuit | BCM | DTC C0277
C0278 | Brake Pedal Position Sensor Not Calibrated | BCM | DTC C0278
C0292 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0460 | Steering Position Signal | EBCM | DTC C0460
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0561 | System Disabled Information Stored | EBCM | DTC C0561
C0569 | System Configuration Error | EBCM | DTC C0569
C0870 | Device Voltage Reference Output 1 Circuit | BCM | DTC C0870
C0899 | Device Voltage Low | EBCM | DTC C0899
C0900 | Device Voltage High | EBCM | DTC C0900
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010 or P0011
P0011 | Intake Camshaft Position (CMP) System Performance | ECM | DTC P0010 or P0011
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0013 or P0014
P0014 | Exhaust Camshaft Position (CMP) System Performance | ECM | DTC P0013 or P0014
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135
P0033 | Turbocharger Bypass Valve Solenoid Control Circuit | ECM | DTC P0033, P0034, or P0035
P0034 | Turbocharger Bypass Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0033, P0034, or P0035
P0035 | Turbocharger Bypass Valve Solenoid Control Circuit High Voltage | ECM | DTC P0033, P0034, or P0035
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0053 | HO2S Heater Resistance Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135
P0087 | Fuel Rail Pressure (FRP) Too Low | ECM | DTC P0087, P0088, or P0089
P0088 | Fuel Rail Pressure (FRP) Too High | ECM | DTC P0087, P0088, or P0089
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0087, P0088, or P0089
P0090 | Fuel Pressure Regulator Control Circuit | ECM | DTC P0090, P0091, or P0092
P0091 | Fuel Pressure Regulator Solenoid 1 Control Circuit Low Voltage | ECM | DTC P0090, P0091, or P0092
P0092 | Fuel Pressure Regulator Solenoid 1 Control Circuit High Voltage | ECM | DTC P0090, P0091, or P0092
P0096 | Intake Air Temperature (IAT) Sensor 2 Performance | ECM | DTC P0096, P0097, P0098, or P0099
P0097 | Intake Air Temperature (IAT) Sensor 2 Circuit Low Voltage | ECM | DTC P0096, P0097, P0098, or P0099
P0098 | Intake Air Temperature (IAT) Sensor 2 Circuit High Voltage | ECM | DTC P0096, P0097, P0098, or P0099
P0099 | Intake Air Temperature (IAT) Sensor 2 Circuit Intermittent | ECM | DTC P0096, P0097, P0098, or P0099
P0100 | Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0101, P0102, or P0103
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0100, P0101, P0102, or P0103
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0101, P0102, or P0103
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0101, P0102, or P0103
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM | DTC P0106, P0107, or P0108
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM | DTC P0106, P0107, or P0108
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM | DTC P0106, P0107, or P0108
P0112 | Intake Air Temperature (IAT) Sensor 1 Circuit Low Voltage | ECM | DTC P0112, P0113, or P0114
P0113 | Intake Air Temperature (IAT) Sensor 1 Circuit High Voltage | ECM | DTC P0112, P0113, or P0114
P0114 | Intake Air Temperature (IAT) Sensor 1 Circuit Intermittent | ECM | DTC P0112, P0113, or P0114
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117, P0118, or P0119
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117, P0118, or P0119
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0117, P0118, or P0119
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, or P0123
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, or P0123
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, or P0123
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control | ECM | DTC P0125 or P0128
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128
P0130 | HO2S Circuit Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P0132 | HO2S Circuit High Voltage Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P0133 | HO2S Slow Response Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P0135 | HO2S Heater Performance Sensor 1 | ECM | DTC P0030, P0031, P0032, P0053, or P0135
P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P0138 | HO2S Circuit High Voltage Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P0141 | HO2S Heater Performance Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0192 | Fuel Rail Pressure (FRP) Sensor Circuit Low Voltage | ECM | DTC P0192 or P0193
P0193 | Fuel Rail Pressure (FRP) Sensor Circuit High Voltage | ECM | DTC P0192 or P0193
P0201 | Injector 1 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0202 | Injector 2 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0203 | Injector 3 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0204 | Injector 4 Control Circuit | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0221, P0222, or P0223
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0221, P0222, or P0223
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0221, P0222, or P0223
P0234 | Turbocharger Engine Overboost | ECM | DTC P0234 or P0299
P0236 | Turbocharger Boost Sensor Performance | ECM | DTC P0236, P0237, or P0238
P0237 | Turbocharger Boost Sensor Circuit Low Voltage | ECM | DTC P0236, P0237, or P0238
P0238 | Turbocharger Boost Sensor Circuit High Voltage | ECM | DTC P0236, P0237, or P0238
P0243 | Turbocharger Wastegate Solenoid Control Circuit | ECM | DTC P0243, P0245, or P0246
P0245 | Turbocharger Wastegate Solenoid Control Circuit Low Voltage | ECM | DTC P0243, P0245, or P0246
P0246 | Turbocharger Wastegate Solenoid Control Circuit High Voltage | ECM | DTC P0243, P0245, or P0246
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P0299 | Turbocharger Engine Underboost | ECM | DTC P0234 or P0299
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0304
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304
P0324 | Knock Sensor (KS) Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0326 | Knock Sensor (KS) 1 Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0327 | Knock Sensor (KS) 1 Circuit Low Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0328 | Knock Sensor (KS) 1 Circuit High Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0331 | Knock Sensor (KS) 2 Performance | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0332 | Knock Sensor (KS) 2 Circuit Low Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0333 | Knock Sensor (KS) 2 Circuit High Voltage | ECM | DTC P0324, P0326, P0327, P0328, P0331, P0332, or P0333
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335, P0336, or P0338
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335, P0336, or P0338
P0338 | Crankshaft Position (CKP) Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338
P0341 | Intake Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341, P0342, or P0343
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM | DTC P0341, P0342, or P0343
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage | ECM | DTC P0341, P0342, or P0343
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance | ECM | DTC P0366, P0367, or P0368
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM | DTC P0366, P0367, or P0368
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage | ECM | DTC P0366, P0367, or P0368
P0420 | Catalyst System Low Efficiency | ECM | DTC P0420
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM | DTC P0446
P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451, P0452, or P0453
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0451, P0452, or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0451, P0452, or P0453
P0455 | Evaporative Emission (EVAP) System Large Leak | ECM | DTC P0455
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Sensor 1 Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Speed Output Circuit | ECM | DTC P0480, P0691, or P0692
P0496 | Evaporative Emission System Flow During Non-Purge | ECM | DTC P0496
P0498 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0502 | Vehicle Speed Sensor (VSS) Circuit Low Voltage | ECM | DTC P0502
P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM | DTC P0503
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507
P0507 | Idle Speed High | ECM | DTC P0506 or P0507
P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0556 | Brake Booster Pressure Sensor Performance | ECM | DTC P0556
P0557 | Brake Booster Pressure Sensor Circuit Low | ECM | DTC P0557
P0058 | Brake Booster Pressure Sensor Circuit High Voltage | ECM | DTC P0558
P0560 | System Voltage | ECM | DTC P0560
P0562 | System Voltage Low | ECM | DTC P0562
P0563 | System Voltage High | ECM | DTC P0563
P0571 | Cruise Control Brake Switch Circuit | ECM | DTC P0571
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0573
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P0602 | Control Module Not Programmed | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P0603 | Control Module Long Term Memory Reset | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P0606 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P0626 | Generator F-Terminal Circuit High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0642 | 5-Volt Reference 1 Low Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0643 | 5-Volt Reference 1 High Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0652 | 5-Volt Reference 2 Low Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0653 | 5-Volt Reference 2 High Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0691 | Cooling Fan Speed Output Circuit Low Voltage | ECM | DTC P0480, P0691, or P0692
P0692 | Cooling Fan Speed Output Circuit High Voltage | ECM | DTC P0480, P0691, or P0692
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0698 | 5-Volt Reference 3 Low Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0699 | 5-Volt Reference 3 High Voltage | ECM | DTC P0641, P0642, P0643, P0651, P0652, P0653, P0697, P0698 or P0699
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700
P0833 | Clutch Pedal Switch 2 Circuit | ECM | DTC P0833
P1011 | Intake Camshaft Position (CMP) Actuator Park Position | ECM | DTC P1011
P1012 | Exhaust Camshaft Position (CMP) Actuator Park Position | ECM | DTC P1012
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176
P1629 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1632 | Theft Deterrent Fuel Disable Signal Received | ECM | DTC P1632
P167A | Control Module HO2S 1 System Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P167D | Control Module Ignition Coil Internal Circuit | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P2088 or P2089
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage | ECM | DTC P2088 or P2089
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P2090 or P2091
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage | ECM | DTC P2090 or P2091
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176
P2101 | Throttle Actuator Position Performance | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P2107 | Throttle Actuator Control (TAC) Module Internal Circuit | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122 or P2123
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122 or P2123
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2127 or P2128
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2127 or P2128
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2138
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P2152 | Injector Positive Voltage Control Circuit Group 3 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P2155 | Injector Positive Voltage Control Circuit Group 4 | ECM | DTC P0201-P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, or P2146-P2157
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P0638, P1551, P2100, P2101, P2119, or P2176
P2177 | Fuel Trim System Lean at Cruise or Accel | ECM | DTC P2177 or P2187
P2178 | Fuel Trim System Rich at Cruise or Accel | ECM | DTC P2178 or P2188
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P2177 or P2187
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P2178 or P2188
P2195 | HO2S Signal Biased Lean Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2196 | HO2S Signal Biased Rich Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2199 | Intake Air Temperature (IAT) Sensor 1-2 Correlation | ECM | DTC P2199
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2227, P2228, or P2229
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2227, P2228, or P2229
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P2237 | HO2S Pumping Current Control Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626
P2243 | HO2S Reference Voltage Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626
P2251 | HO2S Low Reference Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626
P2261 | Turbocharger Bypass Valve Stuck | ECM | DTC P2261
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM | DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
P2297 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2500 | Generator L-Terminal Circuit Low Voltage | ECM | DTC P2500
P2501 | Generator L-Terminal Circuit High Voltage | ECM | DTC P2501
P2535 | Ignition 1 Switch Circuit High Voltage | ECM | DTC P2535
P2544 | Transmission Torque Request Circuit | ECM | DTC P2544
P258A | Vacuum Pump Relay Control Circuit | ECM | DTC P258A-P258D
P258B | Vacuum Pump Performance | ECM | DTC P258A-P258D
P258C | Vacuum Pump Relay Control Circuit Low Voltage | ECM | DTC P258A-P258D
P258D | Vacuum Pump Relay Control Circuit High Voltage | ECM | DTC P258A-P258D
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P062B, P167A, P167D, P2105, P2107, or P2610
P2626 | HO2S Pumping Current Trim Circuit Sensor 1 | ECM | DTC P2237, P2243, P2251, or P2626
U0001 | High Speed CAN Communication Bus | ECM | DTC U0001
U0020 | Low Speed CAN Communication Bus Performance | Radio, RCDLR, VCIM | DTC U0020
U0073 | Controller Area Network (CAN) Bus Communication | ECM, Radio, RCDLR, VCIM | DTC U0073 or U2100
U0100 | Lost Communication With Engine Control Module (ECM) | Radio | DTC U0100-U0299 or U2105-U2199
U0121 | Lost Communication With Antilock Brake Module (ABS) | ECM | DTC U0100-U0299 or U2105-U2199
U0140 | Lost Communication With Body Control Module (BCM) | ECM, VCIM | DTC U0100-U0299 or U2105-U2199
U2100 | Controller Area Network (CAN) Bus Communication | BCM, DRR, EBCM, IPC, RCDLR, SDM, TDM, VCIM | DTC U0073 or U2100
U2103 | Fewer Controllers On Bus Than Programmed | BCM, DRR, IPC, SDM, VCIM | DTC U2103
U2105 | Lost Communications With Engine Control System | BCM, EBCM, TDM | DTC U0100-U0299 or U2105-U2199
U2107 | Lost Communications With Body Control System | EBCM, IPC, RCDLR, TDM | DTC U0100-U0299 or U2105-U2199
U2108 | Lost Communications With ABS/TCS Control System | BCM | DTC U0100-U0299 or U2105-U2199
U2111 | Lost Communications With Steering Control System | BCM | DTC U0100-U0299 or U2105-U2199
U2113 | Lost Communications With Sensing Diagnostic Module (SDM) | BCM, IPC | DTC U0100-U0299 or U2105-U2199
U2116 | Lost Communications With Instrument Panel Cluster (IPC) | BCM | DTC U0100-U0299 or U2105-U2199
U2125 | Lost Communication With Mobile Communications Control Systems | BCM | DTC U0100-U0299 or U2105-U2199
U2137 | Lost Communications With Vehicle Theft Deterrent (VTD) | BCM | DTC U0100-U0299 or U2105-U2199
U2172 | Lost Communications With Digital Radio Receiver | BCM | DTC U0100-U0299 or U2105-U2199
1049 | PPS System Fault Supply Voltage Low | PPS | DTC 1049-1050
1050 | PPS System Fault Supply Voltage High | PPS | DTC 1049-1050
1051 | PPS Initialization/Preload Fault | PPS | DTC 1051
1052 | PPS Preload Failure Region 1 | PPS | DTC 1052, 1053, 1054, or 1055
1053 | PPS Preload Failure Region 2 | PPS | DTC 1052, 1053, 1054, or 1055
1054 | PPS Preload Failure Region 3 | PPS | DTC 1052, 1053, 1054, or 1055
1055 | PPS Preload Failure Region 4 | PPS | DTC 1052, 1053, 1054, or 1055
1058-1062 | PPS Communication Fault | PPS | DTC 1058-1062
1063 | Discard System | PPS | DTC 1063
2036 | Internal Electronic Performance 2 | PPS | DTC 2036-2045
3011 | Internal Electronic Performance 1 | PPS | DTC 3011-3035