For 1990-2009 cars

Connector 1: | Inside Rearview Mirror
Connector 2: | Outside Rearview Mirror - Driver (D48)
Connector 3: | Outside Rearview Mirror - Passenger (D48)
Connector 4: | Outside Rearview Mirror Switch (D48)

### Inside Rearview Mirror

#### Connector Part Information

- OEM: 12124782
- Description: 7-Way F VH Series (BK)

#### Inside Rearview Mirror

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BK | 550 | Ground
3-5 | -- | -- | Not Used
6 | 0.5 GY | 157 | Courtesy Lamp Control
7 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage

### Outside Rearview Mirror - Driver (D48)

#### Connector Part Information

- OEM: E-5965-003
- Description: 3-Way M 1.5 Series, Sealed (BK)

#### Outside Rearview Mirror - Driver (D48)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.35 WH | 81 | Driver Mirror Motor Left Control
2 | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
3 | 0.35 L-GN | 89 | Driver Mirror Motor Up Control

### Outside Rearview Mirror - Passenger (D48)

#### Connector Part Information

- OEM: E-5965-003
- Description: 3-Way M 1.5 Series, Sealed (BK)

#### Outside Rearview Mirror - Passenger (D48)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control
2 | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
3 | 0.35 PU/WH | 889 | Passenger Mirror Motor Up Control

### Outside Rearview Mirror Switch (D48)

#### Connector Part Information

- OEM: 12064769
- Description: 10-Way F Metri-Pack 150 Series (NA)

#### Outside Rearview Mirror Switch (D48)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK | 550 | Ground
C | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
D | 0.35WH | 81 | Driver Mirror Motor Right Control
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
F | 0.35 L-GN | 89 | Driver Mirror Motor Down Control
G | 0.35 RD/WH | 440 | Battery Positive Voltage
H | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
J | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control
K | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control