For 1990-2009 cars

Connector 1: | Audio Amplifier - X1 (UQ3)
Connector 2: | Audio Amplifier - X2 (UQ3)
Connector 3: | Audio Amplifier - X3 (UQ3)
Connector 4: | Digital Radio Receiver (U2K)
Connector 5: | Radio - X1
Connector 6: | Radio - X2
Connector 7: | Speaker - Left Front Door (UQ3)
Connector 8: | Speaker - Left Front Door (UW5)
Connector 9: | Speaker - Left Tweeter
Connector 10: | Speaker - Left Rear (UQ3)
Connector 11: | Speaker - Left Rear (UW5)
Connector 12: | Speaker - Right Front Door (UQ3)
Connector 13: | Speaker - Right Front Door (UW5)
Connector 14: | Speaker - Right Tweeter
Connector 15: | Speaker - Right Rear (UQ3)
Connector 16: | Speaker - Right Rear (UW5)
Connector 17: | Speaker - Subwoofer (UQ3)

### Audio Amplifier - X1 (UQ3)

#### Connector Part Information

- OEM: 15134093
- Description: 8-Way F (BK)

#### Audio Amplifier - X1 (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.0 RD/WH | 640 | Battery Positive Voltage
2 | 2.0 BK/WH | 751 | Ground
3 | 0.8 D-BU/WH | 346 | Left/Rear Subwoofer Speaker Output (+)
4 | 0.8 L-GN/BK | 1794 | Left/Rear Subwoofer Speaker Output (-)
5-6 | -- | -- | Not Used
7 | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
8 | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+)

### Audio Amplifier - X2 (UQ3)

#### Connector Part Information

- OEM: 15134091
- Description: 16-Way F (BK)

#### Audio Amplifier - X2 (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.8 YE | 1956 | Left Front Tweeter Speaker Output (-)
2 | 0.8 TN | 1856 | Left Front Tweeter Speaker Output (+)
3 | 0.8 PU | 1952 | Right Front Tweeter Speaker Output (-)
4 | 0.8 L-GN | 1852 | Right Front Tweeter Speaker Output (+)
5 | 0.8 YE | 116 | Left Rear Speaker Signal Output (-)
6 | 0.8 BN | 199 | Left Rear Speaker Output (+)
7 | 0.8 L-BU | 115 | Right Rear Speaker Signal Output (-)
8 | 0.8 D-BU | 46 | Right Rear Speaker Output (+)
9-12 | -- | -- | Not Used
13 | 1.0 L-GN | 200 | Right Front Speaker Output (+)
14 | 1.0 D-GN | 117 | Right Front Speaker Signal Output (-)
15 | 1.0 TN | 201 | Left Front Speaker Output (+)
16 | 1.0 GY | 118 | Left Front Speaker Signal Output (-)

### Audio Amplifier - X3 (UQ3)

#### Connector Part Information

- OEM: 15136073
- Description: 16-Way F (BK)

#### Audio Amplifier - X3 (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+)
2 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-)
3 | 0.5 BN | 1999 | Left Rear Low Level Audio Signal (-)
4 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal
5 | -- | -- | Not Used
6 | 0.35 PK | 314 | Radio On Signal
7-8 | -- | -- | Not Used
9 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-)
10 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
11 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+)
12 | 0.5 TN | 1946 | Right Rear Low Level Audio Signal (-)
13-15 | -- | -- | Not Used
16 | 0.35 L-GN | 1011 | Remote Radio Control Signal

### Digital Radio Receiver (U2K)

#### Connector Part Information

- OEM:7283-9076-30
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Digital Radio Receiver (U2K)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BN/WH | 367 | Left Audio Signal (+)
3 | 0.5 D-GN/WH | 368 | Right Audio Signal (+)
4 | -- | -- | Not Used
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-8 | -- | -- | Not Used
9 | 0.5 BK/WH | 551 | Ground
10 | 0.5 TN/WH | 372 | Audio Common
11 | 0.35 BK | 814 | Drain
12-15 | -- | -- | Not Used
16 | 0.5 RD/WH | 1340 | Battery Positive Voltage

### Radio - X1

#### Connector Part Information

- OEM: 7283-9076-30
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Radio - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 367 | Left Audio Signal (+) (U2K w/UQ3)
2 | 0.5 D-GN/WH | 368 | Right Audio Signal (+) (U2K w/UQ3)
3 | 0.35 PK | 314 | Radio On Signal (UQ3)
4 | 0.5 L-BU | 115 | Right Rear Speaker Output (-) (UW5)
0.5 TN | 1946 | Right Rear Low Level Audio Signal (-) (UQ3)
5 | 0.5 D-BU | 46 | Right Rear Speaker Output (+) (UW5)
0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+) (UQ3)
6 | 0.5 YE | 116 | Left Rear Speaker Output (-) (UW5)
0.5 BN | 1999 | Left Rear Low Level Audio Signal (-) (UQ3)
7 | 0.5 BN | 199 | Left Rear Speaker Output (+) (UW5)
0.5 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (UQ3)
8 | -- | -- | Not Used
9 | 0.5 TN/WH | 372 | Audio Common (U2K w/UQ3)
10-13 | -- | -- | Not Used
14 | 0.35 WH/BK | 644 | 10-Volt Reference (UK3)
15 | 0.35 L-GN | 1011 | Remote Radio Control Signal (UQ3)
16 | -- | -- | Not Used

### Radio - X2

#### Connector Part Information

- OEM: 7283-4490-30
- Description: 14-Way F (BK)

#### Radio - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.8 RD/WH | 1140 | Battery Positive Voltage
2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
3 | -- | -- | Not Used
4 | 0.5 D-GN | 117 | Right Front Speaker Output (-) (UW5)
0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-) (UQ3)
5 | 0.5 L-GN | 200 | Right Front Speaker Output (+) (UW5)
0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+) (UQ3)
6 | 0.5 GY | 118 | Left Front Speaker Output (-) (UW5)
0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-) (UQ3)
7 | 0.5 TN | 201 | Left Front Speaker Output (+) (UW5)
0.5 TN | 511 | Left Front Low Level Audio Signal (+) (UQ3)
8 | 0.8 BK/WH | 551 | Ground
9 | 0.35 D-GN/WH | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.35 D-BU | 1796 | Steering Column Controls Signal
12-14 | -- | -- | Not Used

### Speaker - Left Front Door (UQ3)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Left Front Door (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-)
B | 0.8 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Front Door (UW5)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Left Front Door (UW5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-)
B | 0.8 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Tweeter

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Left Tweeter

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 TN | 1856 | Left Front Tweeter Speaker Output (+) (UQ3)
0.8 GY | 118 | Left Front Speaker Output (-) (UW5)
B | 0.8 YE | 1956 | Left Front Tweeter Speaker Output (-) (UQ3)
0.8 TN | 201 | Left Front Speaker Output (+) (UW5)

### Speaker - Left Rear (UQ3)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Left Rear (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 YE | 116 | Left Rear Speaker Output (-)
B | 0.8 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Left Rear (UW5)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Left Rear (UW5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 YE | 116 | Left Rear Speaker Output (-)
B | 0.5 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Right Front Door (UQ3)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Right Front Door (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 D-GN | 117 | Right Front Speaker Output (-)
B | 0.8 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Front Door (UW5)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Right Front Door (UW5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 D-GN | 117 | Right Front Speaker Output (-)
B | 0.8 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Tweeter

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Right Tweeter

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 L-GN | 1852 | Right Front Tweeter Speaker Output (+) (UQ3)
0.8 D-GN | 117 | Right Front Speaker Output (-) (UW5)
B | 0.8 PU | 1952 | Right Front Tweeter Speaker Output (-) (UQ3)
0.8 L-GN | 200 | Right Front Speaker Output ( ) (UW5)

### Speaker - Right Rear (UQ3)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Right Rear (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 L-BU | 115 | Right Rear Speaker Output (-)
B | 0.8 D-BU | 46 | Right Rear Speaker Output (+)

### Speaker - Right Rear (UW5)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Right Rear (UW5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 L-BU | 115 | Right Rear Speaker Output (-)
B | 0.5 D-BU | 46 | Right Rear Speaker Output (+)

### Speaker - Subwoofer (UQ3)

#### Connector Part Information

- OEM: 12064760
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Speaker - Subwoofer (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
B | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+)
C | 0.8 L-GN/BK | 1794 | Left/Rear Subwoofer Speaker Output (-)
D | 0.8 D-BU/WH | 346 | Left/Rear Subwoofer Speaker Output (+)