For 1990-2009 cars

Connector 1: | A/C Compressor Clutch (C60)
Connector 2: | A/C Refrigerant Pressure Sensor (C60)
Connector 3: | Accelerator Pedal Position (APP) Sensor
Connector 4: | Accessory Power Outlet
Connector 5: | Air Temperature Actuator - Left
Connector 6: | Air Temperature Actuator - Right
Connector 7: | Ambient Light Sensor
Connector 8: | Audio Amplifier - X1 (UQ3)
Connector 9: | Audio Amplifier - X2 (UQ3)
Connector 10: | Audio Amplifier - X3 (UQ3)
Connector 11: | Backup Lamp
Connector 12: | Backup Lamp Switch
Connector 13: | Blower Motor
Connector 14: | Blower Motor High Speed Relay
Connector 15: | Blower Motor Resistor
Connector 16: | Body Control Module (BCM) X1
Connector 17: | Body Control Module (BCM) X2
Connector 18: | Body Control Module (BCM) X3
Connector 19: | Body Control Module (BCM) X4
Connector 20: | Brake Booster Pump Motor (Late Production)
Connector 21: | Brake Booster Vacuum Sensor
Connector 22: | Brake Fluid Level Switch
Connector 23: | Brake Pedal Position (BPP) Sensor
Connector 24: | Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust
Connector 25: | Camshaft Position (CMP) Actuator Solenoid Valve - Intake
Connector 26: | Camshaft Position (CMP) Sensor - Exhaust
Connector 27: | Camshaft Position (CMP) Sensor - Intake
Connector 28: | Center High Mounted Stop Lamp (CHMSL)
Connector 29: | Cigar Lighter X1
Connector 30: | Cigar Lighter X2
Connector 31: | Clutch Pedal Position (CPP) Sensor (MA5)
Connector 32: | Crankshaft Position (CKP) Sensor
Connector 33: | Data Link Connector (DLC)
Connector 34: | Data Link Resistor
Connector 35: | Door Lock Actuator - Driver (AU3)
Connector 36: | Door Lock Actuator - Passenger (AU3)
Connector 37: | Door Lock Switch - Driver (AU3)
Connector 38: | Door Lock Switch - Passenger (AU3)
Connector 39: | Electronic Brake Control Module (EBCM) (JL9)
Connector 40: | Engine Control Module (ECM) X1
Connector 41: | Engine Control Module (ECM) X2
Connector 42: | Engine Coolant Level Switch
Connector 43: | Engine Coolant Temperature (ECT) Sensor
Connector 44: | Engine Cooling Fan
Connector 45: | Engine Oil Pressure (EOP) Switch
Connector 46: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 47: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
Connector 48: | Evaporator Temperature Sensor (C60)
Connector 49: | Fog Lamp - Left Front (T96)
Connector 50: | Fog Lamp - Rear (T79)
Connector 51: | Fog Lamp - Right Front (T96)
Connector 52: | Fog Lamp Switch - Front (T96)
Connector 53: | Fog Lamp Switch - Rear (T79)
Connector 54: | Folding Top Cover Actuator
Connector 55: | Fuel Injector 1
Connector 56: | Fuel Injector 2
Connector 57: | Fuel Injector 3
Connector 58: | Fuel Injector 4
Connector 59: | Fuel Pump and Sender Assembly
Connector 60: | Fuel Rail Pressure (FRP) Sensor
Connector 61: | Fuel Tank Pressure (FTP) Sensor
Connector 62: | Generator X1
Connector 63: | Generator X2
Connector 64: | Hazard Warning Switch
Connector 65: | Headlamp - Left High Beam
Connector 66: | Headlamp - Left Low Beam
Connector 67: | Headlamp - Right High Beam
Connector 68: | Headlamp - Right Low Beam
Connector 69: | Heated Oxygen Sensor (HO2S) 1
Connector 70: | Heated Oxygen Sensor (HO2S) 2
Connector 71: | High Pressure Fuel Pump
Connector 72: | Horn - Left
Connector 73: | Horn - Right
Connector 74: | Horn Switch
Connector 75: | HVAC Control Module X1
Connector 76: | HVAC Control Module X2
Connector 77: | HVAC Control Module X3
Connector 78: | I/P Dimmer Switch
Connector 79: | Ignition Coil 1
Connector 80: | Ignition Coil 2
Connector 81: | Ignition Coil 3
Connector 82: | Ignition Coil 4
Connector 83: | Ignition Switch
Connector 84: | Inflatable Restraint Front End Sensor - Left
Connector 85: | Inflatable Restraint Front End Sensor - Right
Connector 86: | Inflatable Restraint I/P Module X1
Connector 87: | Inflatable Restraint I/P Module X2
Connector 88: | Inflatable Restraint I/P Module Indicator
Connector 89: | Inflatable Restraint Passenger Presense System (PPS) Module
Connector 90: | Inflatable Restraint Sensing and Diagnostic Module (SDM)
Connector 91: | Inflatable Restraint Steering Wheel Module X1
Connector 92: | Inflatable Restraint Steering Wheel Module X2
Connector 93: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 94: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 95: | Inflatable Restraint Steering Wheel Module Coil X3
Connector 96: | Inside Rearview Mirror (ISRVM)
Connector 97: | Instrument Panel Cluster (IPC)
Connector 98: | Intake Air Pressure and Temperature Sensor
Connector 99: | Knock Sensor (KS) - 1
Connector 100: | Knock Sensor (KS) - 2
Connector 101: | License Lamp - Left
Connector 102: | License Lamp - Right
Connector 103: | Manifold Absolute Pressure (MAP) Sensor
Connector 104: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 105: | Mode Actuator
Connector 106: | Outside Air Temperature Sensor
Connector 107: | Outside Rearview Mirror - Driver (D48)
Connector 108: | Outside Rearview Mirror - Passenger (D48)
Connector 109: | Outside Rearview Mirror Switch (D48)
Connector 110: | Park Brake Switch
Connector 111: | Park Lamp - Left Front
Connector 112: | Park Lamp - Right Front
Connector 113: | Radio - X1
Connector 114: | Radio - X2
Connector 115: | Rear Compartment Courtesy Lamp
Connector 116: | Rear Compartment Lid Ajar Switch
Connector 117: | Rear Compartment Lid Release Actuator
Connector 118: | Rear Compartment Lid Release Switch
Connector 119: | Rear Window Defogger Grid X1
Connector 120: | Rear Window Defogger Grid X2
Connector 121: | Recirculation Actuator
Connector 122: | Remote Control Door Lock Receiver (RCDLR) (AU3/AU0)
Connector 123: | Seat Adjuster Switch - Driver (AF2)
Connector 124: | Seat Belt Pretensioner - Driver
Connector 125: | Seat Belt Pretensioner - Passenger
Connector 126: | Seat Belt Switch - Driver
Connector 127: | Seat Belt Switch - Passenger
Connector 128: | Seat Front Vertical Motor - Driver (AF2)
Connector 129: | Speaker - Left Front (UQ3)
Connector 130: | Speaker - Left Front (UW5)
Connector 131: | Speaker - Left Rear (UQ3)
Connector 132: | Speaker - Left Rear (UW5)
Connector 133: | Speaker - Left Tweeter
Connector 134: | Speaker - Right Front (UQ3)
Connector 135: | Speaker - Right Front (UW5)
Connector 136: | Speaker - Right Rear (UQ3)
Connector 137: | Speaker - Right Rear (UW5)
Connector 138: | Speaker - Right Tweeter
Connector 139: | Speaker - Subwoofer (UQ3)
Connector 140: | Starter Motor X1
Connector 141: | Starter Motor X2
Connector 142: | Steering Angle Sensor (JL9)
Connector 143: | Steering Wheel Control Switch - Left (K34)
Connector 144: | Steering Wheel Control Switch - Right (UK3)
Connector 145: | Tail/Stop Lamp - Left
Connector 146: | Tail/Stop Lamp - Right
Connector 147: | Theft Deterrent Module (TDM)
Connector 148: | Throttle Body
Connector 149: | Traction Control Switch (TCS) (JL9)
Connector 150: | Turbocharger Bypass Valve Solenoid
Connector 151: | Turbocharger Wastegate Solenoid
Connector 152: | Turn Signal Lamp - Left Front
Connector 153: | Turn Signal Lamp - Right Front
Connector 154: | Turn Signal Lamp - Left Rear
Connector 155: | Turn Signal Lamp - Right Rear
Connector 156: | Turn Signal Repeater - Left
Connector 157: | Turn Signal Repeater - Right
Connector 158: | Turn Signal/Multifunction Switch X1
Connector 159: | Turn Signal/Multifunction Switch X2
Connector 160: | Vehicle Speed Sensor (VSS) (MA5)
Connector 161: | Wheel Speed Sensor (WSS) - Left Front
Connector 162: | Wheel Speed Sensor (WSS) - Left Rear
Connector 163: | Wheel Speed Sensor (WSS) - Right Front
Connector 164: | Wheel Speed Sensor (WSS) - Right Rear
Connector 165: | Window Motor - Driver (A31)
Connector 166: | Window Motor - Passenger (A31)
Connector 167: | Window Switch - Driver (A31)
Connector 168: | Window Switch - Passenger (A31)
Connector 169: | Windshield Washer Fluid Pump
Connector 170: | Windshield Wiper Motor
Connector 171: | Windshield Wiper/Washer Switch
Connector 172: | Yaw and Lateral Accelerometer Sensor (JL9)

### A/C Compressor Clutch (C60)

#### Connector Part Information

- OEM: 12052644
- Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### A/C Compressor Clutch (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 250 | Ground
B | 0.5 D-GN | 59 | A/C Compressor Clutch Supply Voltage

### A/C Refrigerant Pressure Sensor (C60)

#### Connector Part Information

- OEM: 15477863
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### A/C Refrigerant Pressure Sensor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 5514 | Low Reference
2 | 0.35 GY | 2700 | 5-Volt Reference 3
3 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15397577
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | Low Reference
B | 0.35 L-BU | 1162 | Throttle Position Sensor 2 Signal
C | 0.35 TN | 1274 | 5-Volt Reference 3
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | Throttle Position Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference 2

### Accessory Power Outlet

#### Connector Part Information

- OEM: 12176836
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Accessory Power Outlet

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 RD/WH | 240 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1.0 BK | 550 | Ground

### Air Temperature Actuator - Left

#### Connector Part Information

- OEM: 12064982
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Air Temperature Actuator - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
3 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
4 | 0.35 D-BU | 1199 | Air Temperature Door Control
5 | 0.35 L-GN/BK | 1647 | Air Temperature Door Control

### Air Temperature Actuator - Right

#### Connector Part Information

- OEM: 12064982
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Air Temperature Actuator - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 D-BU | 1646 | Air Temperature Door Position Signal
3 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
4 | 0.35 L-GN/BK | 1647 | Air Temperature Door Control
5 | 0.35 TN | 2273 | Mode Door Control

### Ambient Light Sensor

#### Connector Part Information

- OEM: 12047662
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Ambient Light Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 1137 | Daytime Running Lights Ambient Light Sensor Signal
B | 0.35 YE/BK | 1138 | Low Reference

### Audio Amplifier - X1 (UQ3)

#### Connector Part Information

- OEM: 6098-4713
- Description: 8-Way F (BK)

#### Audio Amplifier - X1 (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 RD/WH | 640 | Battery Positive Voltage
2 | 2.0 BK/WH | 751 | Ground
3 | 0.8 D-BU/WH | 346 | Left Subwoofer Speaker Output (+)
4 | 0.8 L-GN/BK | 1794 | Left Subwoofer Speaker Output (-)
5-6 | -- | -- | Not Used
7 | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
8 | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+)

### Audio Amplifier - X2 (UQ3)

#### Connector Part Information

- OEM: 6098-4611
- Description: 16-Way F (BK)

#### Audio Amplifier - X2 (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 YE | 1956 | Left Tweeter Speaker Output (-)
2 | 0.8 TN | 1856 | Left Tweeter Speaker Output (+)
3 | 0.8 PU | 1952 | Right Tweeter Speaker Output (-)
4 | 0.8 L-GN | 1852 | Right Tweeter Speaker Output (+)
5 | 0.8 YE | 116 | Left Rear Speaker Signal Output (-)
6 | 0.8 BN | 199 | Left Rear Speaker Output (+)
7 | 0.8 L-BU | 115 | Right Rear Speaker Signal Output (-)
8 | 0.8 D-BU | 46 | Right Rear Speaker Output (+)
9-12 | -- | -- | Not Used
13 | 1.0 L-GN | 200 | Right Front Speaker Output (+)
14 | 1.0 D-GN | 117 | Right Front Speaker Signal Output (-)
15 | 1.0 TN | 201 | Left Front Speaker Output (+)
16 | 1.0 GY | 118 | Left Front Speaker Signal Output (-)

### Audio Amplifier - X3 (UQ3)

#### Connector Part Information

- OEM: 7283-9076-30
- Description: 16-Way F (BK)

#### Audio Amplifier - X3 (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+)
2 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-)
3 | 0.5 BN | 1999 | Left Rear Low Level Audio Signal (-)
4 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal
5 | -- | -- | Not Used
6 | 0.35 PK | 314 | Radio On Signal
7-8 | -- | -- | Not Used
9 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-)
10 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
11 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+)
12 | 0.5 TN | 1946 | Right Rear Low Level Audio Signal (-)
13-15 | -- | -- | Not Used
16 | 0.35 L-GN | 1011 | Remote Radio Control Signal

### Backup Lamp

#### Connector Part Information

- OEM: 7223-1324-60
- Description: 2-Way F 090 Series (GN)

#### Backup Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
2 | 0.5 BK | 750 | Ground

### Backup Lamp Switch

#### Connector Part Information

- OEM: 12103584
- Description: 2-Way M Weather Pack (BK)

#### Backup Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 PK | 539 | Ignition 1 Voltage
B | 0.8 L-GN | 24 | Backup Lamp Supply Voltage

### Blower Motor

#### Connector Part Information

- OEM: 7283-5590-40
- Description: 2-Way F YESC/USCAR Class III Series (BK)

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 OG | 52 | Blower Motor High Control
2 | 3.0 BN | 141 | Ignition 3 Voltage

### Blower Motor High Speed Relay

#### Connector Part Information

- OEM: 12034003
- Description: 5-Way F Special Metri-Pack 630 Conn (BK)

#### Blower Motor High Speed Relay

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 BK | 2050 | Ground
2 | 3.0 BN | 141 | Ignition 3 Voltage
3 | -- | -- | Not Used
4 | 3.0 OG | 52 | Blower Motor High Control
5 | 3.0 OG | 52 | Blower Motor High Control

### Blower Motor Resistor

#### Connector Part Information

- OEM: 12059296
- Description: 5-Way F Metri-Pack 480 Series (RD)

#### Blower Motor Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 OG | 52 | Blower Motor High Control
B | 2.0 YE | 60 | Blower Motor Low Control
C | 2.0 TN | 63 | Blower Motor Medium 1 Control
D | 2.0 L-BU | 72 | Medium 2 Blower Motor Control
E | 3.0 OG | 52 | Blower Motor High Control

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: 15393122
- Description: 72-Way F Micro-64 Unsealed (BU with GY case)

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.35 YE | 682 | Door Lock/Unlock Signal (AU3)
7 | 0.35 BN | 682 | Door Lock/Unlock Signal (AU3)
8 | 0.35 WH | 1080 | Park Lamp Relay Control
9-12 | -- | -- | Not Used
13 | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
14 | 0.5 L-BU | 1134 | Park Brake Switch Signal
15 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
16 | 0.35 WH | 193 | Rear Defog Relay Control
17 | 0.5 D-BU | 15 | Right Turn Signal Lamps Supply Voltage
18 | -- | -- | Not Used
19 | 0.35 PK/WH | 746 | Right Front Door Ajar Switch Signal
20-21 | -- | -- | Not Used
22 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
23-25 | -- | -- | Not Used
26 | 0.5 L-GN | 1478 | Coolant Level Switch Signal
27-30 | -- | -- | Not Used
31 | 0.35 WH | 5065 | Stop Lamp Relay Coil Supply Voltage
32-34 | -- | -- | Not Used
35 | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
36-39 | -- | -- | Not Used
40 | 0.35 L-BU | 1788 | Traction Control Switch Signal (JL9)
41-43 | -- | -- | Not Used
44 | 0.35 TN/WH | 1969 | Headlamp High Beam Relay Control
45-46 | -- | -- | Not Used
47 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
48-50 | -- | -- | Not Used
51 | 0.35 D-GN | 113 | Windshield Wiper Relay Control
52 | -- | -- | Not Used
53 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
54 | 0.35 YE | 317 | Fog Lamp Relay Control (T96)
55 | 0.35 OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
56 | 0.5 OG/BK | 737 | Rear Compartment Lamp Control
57 | 0.35 BN | 253 | Trunk Release Relay Control
58-59 | -- | -- | Not Used
60 | 0.35 TN | 28 | Horn Relay Control
61 | 0.5 BK/WH | 651 | Ground
62-66 | -- | -- | Not Used
67 | 0.5 YE | 61 | Low Reference
68-69 | -- | -- | Not Used
70 | 0.5 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
71-72 | -- | -- | Not Used

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: 15393121
- Description: 72-Way F Micro-64 Unsealed (GY)

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
3 | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control
4 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
5 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
6 | 0.35 L-BU | 187 | Rear Fog Lamp Switch Signal (T79)
7-8 | -- | -- | Not Used
9 | 0.35 WH | 111 | Hazard Warning Switch Signal
10 | 0.35 TN | 1576 | Rear Compartment Lock Actuator Unlock
11 | 0.35 D-GN | 264 | Security Indicator Supply Voltage
12-13 | -- | -- | Not Used
14 | 0.35 TN | 28 | Horn Relay Control
15 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
16 | 0.35 OG | 192 | Front Fog Lamp Switch Signal (T96)
17 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
18 | 0.35 WH | 5359 | 5-Volt Reference
19 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
20 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
21 | -- | -- | Not Used
22 | 0.35 YE | 1977 | Rear Fog Lamp Relay Control (T79)
21-25 | -- | -- | Not Used
26 | 0.35 D-GN | 44 | I/P Dimmer Switch Lamp Signal
27-30 | -- | -- | Not Used
31 | 0.35 YE | 5361 | Brake Pedal Position Sensor Signal
32 | -- | -- | Not Used
33 | 0.35 YE | 317 | Fog Lamp Relay Control (T96)
34-37 | -- | -- | Not Used
38 | 0.35 L-GN/BK | 5060 | Low Speed GMLAN Serial Data
39-43 | -- | -- | Not Used
44 | 0.35 L-GN/BK | 1137 | Daytime Running Lamp Ambient Light Sensor Signal
45-46 | -- | -- | Not Used
47 | 0.35 YE/BK | 1138 | Low Reference
48-50 | -- | -- | Not Used
51 | 0.35 BN | 1356 | Flash To Pass Switch Signal
52-55 | -- | -- | Not Used
56 | 0.35 WH | 1390 | Off/Run/Crank Voltage
57 | 0.35 GY | 112 | Windshield Wiper Switch Low/Pulse Signal
58 | 0.35 PU | 719 | Low Reference
59 | 0.35 BN | 5360 | Low Reference
60 | -- | -- | Not Used
61 | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
62 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal
63-65 | -- | -- | Not Used
66 | 0.35 YE/BK | 1418 | Left Rear Turn Signal Switch Signal
67 | 0.35 D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
68 | 0.35 L-BU | 292 | Rear Window Defogger Grid Switch Signal
69 | 0.35 D-GN/WH | 762 | A/C Request Signal (C60)
70 | -- | -- | Not Used
71 | 0.35 PU | 5234 | Passenger Seat Belt Indicator
72 | 0.35 WH | 193 | Rear Window Defogger Grid Relay Control

### Body Control Module (BCM) X3

#### Connector Part Information

- OEM: 15492675
- Description: 41-Way F Metri-Pack 280 800 Series (RD)

#### Body Control Module (BCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3)
A2 | -- | -- | Not Used
A3 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
A4 | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3)
A5 | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3)
A6 | -- | -- | Not Used
A7 | 0.5 BN | 9 | Park Lamp Supply Voltage
A8 | 0.5 PK | 339 | Ignition 1 Voltage
A9 | 0.8 YE | 618 | Left Rear Turn Signal Lamp Supply Voltage
A10 | 0.5 GY | 157 | Courtesy Lamp Control
A11 | -- | -- | Not Used
A12 | 0.8 D-GN | 619 | Right Rear Turn Signal Lamp Supply Voltage
B1 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AU3)
B2 | -- | -- | Not Used
B3 | 0.35 RD/WH | 1240 | Battery Positive Voltage
B4 | -- | -- | Not Used
B5 | 0.35 BN | 4 | Accessory Voltage
B6-B7 | -- | -- | Not Available
B8-B11 | -- | -- | Not Used
B12 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C1-C2 | -- | -- | Not Available
C3-C4 | -- | -- | Not Used
C5 | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
C6-C7 | -- | -- | Not Available
C8-C11 | -- | -- | Not Used
C12 | 0.35 OG | 228 | Windshield Washer Pump Control
D1 | 5.0 RD/BK | 142 | Battery Positive Voltage
D2-D3 | -- | -- | Not Used
D4 | 0.5 RD/WH | 840 | Battery Positive Voltage
D5 | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage (AU3)
D6 | 3.0 PK | 739 | Ignition 1 Voltage
D7 | 0.35 PK | 1339 | Ignition 1 Voltage
D8-D9 | -- | -- | Not Used
D10 | 3.0 RD/BK | 442 | Battery Positive Voltage
D11 | 2.0 RD/WH | 640 | Battery Positive Voltage (UQ3)
D12 | 3.0 RD/BK | 242 | Battery Positive Voltage

### Body Control Module (BCM) X4

#### Connector Part Information

- OEM: 15492668
- Description: 68-Way F Metri-Pack 280 Series, Flexlock (L-GY)

#### Body Control Module (BCM) X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1-A12 | -- | -- | Not Used
B1 | 0.35 OG | 228 | Windshield Washer Pump Control
B2-B12 | -- | -- | Not Used
C1 | 0.35 RD/WH | 1440 | Battery Positive Voltage
C2-C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8 | 0.35 BN | 4 | Accessory Voltage
C9-C10 | -- | -- | Not Used
C11 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C12 | 0.35 GY/BK | 1458 | Instrument Panel Lamp Supply Voltage (4)
D1 | 0.35 RD/WH | 1040 | Battery Positive Voltage
D2 | -- | -- | Not Used
D3 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
D4 | 3.0 BN | 141 | Ignition 3 Voltage
D5 | -- | -- | Not Used
D6-D7 | -- | -- | Not Available
D8-D9 | -- | -- | Not Used
D10 | 0.8 RD/WH | 1140 | Battery Positive Voltage
D11-D12 | -- | -- | Not Used
E1-E5 | -- | -- | Not Used
E6 | 0.35 PK | 439 | Ignition 1 Voltage
E7-E11 | -- | -- | Not Used
E12 | 2.0 BK | 550 | Ground
F1 | 0.35 RD/WH | 1540 | Battery Positive Voltage
F2 | 0.5 GY | 8 | Instrument Panel Lamp Supply Voltage
F3 | -- | -- | Not Used
F4 | 0.5 PK | 339 | Ignition 1 Voltage
F5 | 0.35 PK | 339 | Ignition 1 Voltage
F6 | 0.5 PK | 339 | Ignition 1 Voltage
F7-F8 | -- | -- | Not Used
F9 | 0.35 PK | 1539 | Ignition 1 Voltage
F10-F12 | -- | -- | Not Used

### Brake Booster Pump Motor (Late Production)

#### Connector Part Information

- OEM: 7282-5575-10
- Description: 2-Way M 2.8 Series (D-GY)

#### Brake Booster Pump Motor (Late Production)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5OG | 1470 | Brake Booster Pump Motor Supply Voltage
2 | 0.5 BK/WH | 1250 | Ground

### Brake Booster Vacuum Sensor

#### Connector Part Information

- OEM: 1 928 403 966
- Description: 3-Way F Kompakt 2.8 Series, Sealed (BK)

#### Brake Booster Vacuum Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 6257 | Brake Booster Vacuum Sensor Supply Voltage (Early Production)
0.5 L-GN | 6031 | 5-Volt Reference (Late Production)
2 | 0.5 L-GN/BK | 6258 | Brake Booster Vacuum Sensor Ground (Early Production)
0.5 YE/BK | 6032 | Low Reference (Late Production)
3 | 0.5 D-BU | 1809 | Brake Booster Vacuum Sensor Signal (Early Production)
0.5 OG | 6030 | Brake Booster Vacuum Sensor Signal (Late Production)

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 12052641
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 849 | Brake Fluid Level Sensor Signal
B | 0.5 BK/WH | 451 | Ground

### Brake Pedal Position (BPP) Sensor

#### Connector Part Information

- OEM: 15332132
- Description: 3-Way F GT 150 Series (BK)

#### Brake Pedal Position (BPP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 5359 | 5-Volt Reference
B | 0.35 YE | 5361 | Brake Pedal Position Sensor Signal
C | 0.35 BN | 5360 | Low Reference

### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust

#### Connector Part Information

- OEM: 15336004
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply 4
B | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid Control

### Camshaft Position (CMP) Actuator Solenoid Valve - Intake

#### Connector Part Information

- OEM: 15335987
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply 4
B | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid Control

### Camshaft Position (CMP) Sensor - Exhaust

#### Connector Part Information

- OEM: 15326808
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Sensor - Exhaust

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 705 | 5-Volt Reference 2
B | 0.5 TN | 552 | Low Reference
C | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor Signal 1

### Camshaft Position (CMP) Sensor - Intake

#### Connector Part Information

- OEM: 15326808
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Camshaft Position (CMP) Sensor - Intake

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 705 | 5-Volt Reference 2
B | 0.5 TN | 552 | Low Reference
C | 0.5 OG | 5275 | Camshaft Position Intake Sensor Signal

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: 12052644
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 750 | Ground
B | 0.5 L-BU | 20 | Stop Lamp Supply Voltage

### Cigar Lighter X1

#### Connector Part Information

- OEM: 12131237
- Description: 1-Way F Faston 4.8 (BK)

#### Cigar Lighter X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 8 | Instrument Panel Lamp Supply Voltage

### Cigar Lighter X2

#### Connector Part Information

- OEM: 1-926522-1
- Description: 2-Way F Positive Lock Series (BK)

#### Cigar Lighter X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 BK | 550 | Ground
2 | 1.0 RD/WH | 240 | Battery Positive Voltage

### Clutch Pedal Position (CPP) Sensor (MA5)

#### Connector Part Information

- OEM: 15332132
- Description: 3-Way F Metri-Pack 280 Series (BK)

#### Clutch Pedal Position (CPP) Sensor (MA5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-BU/WH | 7361 | Manual Transmission Clutch Position Sensor Supply
B | 0.35 L-GN | 6338 | Manual Transmission Clutch Position Sensor Signal Position
C | 0.35 OG/D-GN | 7360 | Manual Transmission Clutch Position Sensor Return

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 31403-3700 (Delphi # 13521040)
- Description: 3-Way F MX64 Series, Sealed (BK)

#### Crankshaft Position (CKP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 605 | 5-Volt Reference 3
2 | 0.35 TN | 452 | Low Reference
3 | 0.35 YE | 573 | Crankshaft Position Sensor Signal

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 12110250
- Description: 16-Way F Metri-Pack 150 Series (BK)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2-3 | -- | -- | Not Used
4 | 0.5 BK | 550 | Ground
5 | 0.5 BK/WH | 651 | Ground
6 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
7-13 | -- | -- | Not Used
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
15 | -- | -- | Not Used
16 | 0.5 RD/WH | 40 | Battery Positive Voltage

### Data Link Resistor

#### Connector Part Information

- OEM: 13510085
- Description: 2-Way F GT 150 Series (BK)

#### Data Link Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
B | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)

### Door Lock Actuator - Driver (AU3)

#### Connector Part Information

- OEM: 6-1355683-1
- Description: 6-Way F Series Sealed (BK)

#### Door Lock Actuator - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
3 | 0.5 GY | 295 | Door Lock Actuator Lock Control
4 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | 0.35 BK | 550 | Ground

### Door Lock Actuator - Passenger (AU3)

#### Connector Part Information

- OEM: 6-1355683-1
- Description: 6-Way F Series Sealed (BK)

#### Door Lock Actuator - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | 0.35 BK | 550 | Ground
4 | -- | -- | Not Used
5 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
6 | 0.5 GY | 295 | Door Lock Actuator Lock Control

### Door Lock Switch - Driver (AU3)

#### Connector Part Information

- OEM: 15417063
- Description: 3-Way F Micro-Pack 064 Series (BK)

#### Door Lock Switch - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 550 | Ground
B | 0.35 GY | 8 | Instrument Lamp Supply Voltage
C | 0.5 WH | 682 | Door Lock/Unlock Signal

### Door Lock Switch - Passenger (AU3)

#### Connector Part Information

- OEM: 15417063
- Description: 3-Way F Micro-Pack 064 Series (BK)

#### Door Lock Switch - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 550 | Ground
B | 0.35 GY | 8 | Instrument Lamp Supply Voltage
C | 0.5 WH | 682 | Door Lock/Unlock Signal

### Electronic Brake Control Module (EBCM) (JL9)

#### Connector Part Information

- OEM: 6-1355628-1
- Description: 47-Way F MK25/60 Series (BK)

#### Electronic Brake Control Module (EBCM) (JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 RD/BK | 542 | Low Reference
2-7 | -- | -- | Not Used
8 | 0.5 PK | 1439 | Ignition 1 Voltage
9-10 | -- | -- | Not Used
11 | 0.5 TN/BK | 2500 | High Speed Serial Data Bus (+)
12 | 0.5 TN/BK | 2500 | High Speed Serial Data Bus (+)
13 | 0.5 TN | 2501 | High Speed Serial Data Bus (-)
14 | 0.5 TN | 2501 | High Speed Serial Data Bus (-)
15 | -- | -- | Not Used
16 | 3.0 BK | 350 | Ground
17 | -- | -- | Not Used
18 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
19 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
20-21 | -- | -- | Not Used
22 | 0.5 D-GN | 2087 | 12-Volt Reference
23-25 | -- | -- | Not Used
26 | 0.5 L-GN | 6257 | Brake Booster Vacuum Sensor Supply Voltage (Early Production)
27 | 0.5 L-GN/BK | 6258 | Brake Booster Vacuum Sensor Ground (Early Production)
28 | -- | -- | Not Used
29 | 0.5 L-BU | 2088 | Low Reference
30-31 | -- | -- | Not Used
32 | 2.0 RD/WH | 540 | Battery Positive Voltage
33 | 0.5 TN | 833 | Low Reference
34 | 0.5 D-GN | 872 | Wheel Speed Sensor Signal (WSS) - Right Front
35 | -- | -- | Not Used
36 | 0.5 TN | 884 | Wheel Speed Sensor Signal (WSS) - Left Rear
37 | 0.5 OG | 885 | Low Reference
38-40 | -- | -- | Not Used
41 | 0.5 D-BU | 1809 | Brake Booster Vacuum Sensor Signal (Early Production)
42 | 0.5 WH | 883 | Low Reference
43 | 0.5 BN | 882 | Wheel Speed Sensor Signal (WSS) - Right Rear
44 | -- | -- | Not Used
45 | 0.5 L-BU | 830 | Wheel Speed Sensor Signal (WSS) - Left Front
46 | 0.5 YE | 873 | Low Reference
47 | -- | -- | Not Used

### Engine Control Module (ECM) X1

#### Connector Part Information

- OEM: 1 928 404 781
- Description: 96-Way F Sealed (BK)

#### Engine Control Module (ECM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid Control
2 | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid Control
3-4 | -- | -- | Not Used
5 | 1.0 YE | 7301 | High Pressure Fuel Pump Actuator High Control
6 | 0.5 D-GN/WH | 428 | Evaporative Emission (EVAP) Canister Purge Solenoid Control
7 | 0.5 OG | 5275 | Camshaft Position Intake Sensor Signal
8-9 | -- | -- | Not Used
10 | 0.35 OG | 225 | Generator Turn On Signal
11-12 | -- | -- | Not Used
13 | 0.35 BN/WH | 2130 | Low Reference
14 | -- | -- | Not Used
15 | 0.5 GY | 705 | 5-Volt Reference 2
16 | 0.5 D-GN | 6391 | Turbocharger Bypass Valve Control
17 | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
18 | 0.5 YE | 258 | Turbocharger Wastegate Solenoid Control
19-23 | -- | -- | Not Used
24 | 0.8 YE | 581 | Throttle Actuator Control Motor Control - 1
25 | -- | -- | Not Used
26 | 1.0 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
27 | 1.0 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4
28 | 1.0 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
29 | 1.0 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2
30 | 0.35 GY | 23 | Generator Field Duty Cycle Signal
31-33 | -- | -- | Not Used
34 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor Signal 1
35 | 0.35 YE | 573 | Crankshaft Position (CKP) Sensor Signal
36 | 0.5 YE | 2918 | Fuel Rail Pressure Sensor Signal
37 | 0.5 L-GN | 432 | Manifold Absolute Pressure Sensor Signal
38 | 0.5 GY | 598 | 5-Volt Reference 1
39 | 0.5 GY | 2701 | 5-Volt Reference 3
40 | 0.5 GY | 6031 | 5-Volt Reference (Late Production)
41 | 0.5 TN | 552 | Low Reference
42 | 0.5 TN | 808 | Low Reference
43 | 0.5 YE/BK | 6032 | Low Reference (Late Production)
44 | 0.5 TN | 2761 | Low Reference
45 | 0.5 GY | 605 | 5-Volt Reference 3
46 | 0.35 TN | 452 | Low Reference
47 | -- | -- | Not Used
48 | 0.8 BN | 582 | Throttle Actuator Control Motor Control - 2
49-50 | -- | -- | Not Used
51 | 1.0 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
52 | 1.0 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
53 | 1.0 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3
54 | 0.35 BN/WH | 419 | MIL Control
55 | 0.35 PU | 2121 | IC 1 Control
56 | 0.35 D-GN/WH | 2124 | IC 4 Control
57-58 | -- | -- | Not Used
59 | 0.5 D-BU | 496 | Knock Sensor 1 Signal
60 | 0.5 GY | 2303 | Knock Sensor 2 Signal
61-63 | -- | -- | Not Used
64 | 0.5 TN | 407 | Low Reference
65 | -- | -- | Not Used
66 | 0.5 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal
67 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal Sensor 1
68 | 0.5 WH | 5279 | Heated Oxygen Sensor Pump Current Sensor 1
69-72 | -- | -- | Not Used
73 | 1.0 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
74 | -- | -- | Not Used
75 | 1.0 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1
76-77 | -- | -- | Not Used
78 | 0.35 BN | 2129 | Low Reference
79 | 0.35 L-BU | 2123 | IC 3 Control
80 | 0.35 OG/WH | 2122 | IC 2 Control
81 | -- | -- | Not Used
82 | 0.5 YE | 410 | Engine Coolant Temperature Sensor Signal
83 | 0.5 GY | 1716 | Knock Sensor 1 Signal
84 | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
85 | -- | -- | Not Used
86 | 0.5 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
87 | -- | -- | Not Used
88 | 0.5 TN | 2752 | Low Reference
89 | 0.5 PU | 486 | Throttle Position Sensor 2 Signal
90 | 0.5 D-GN | 485 | Throttle Position Sensor 1 Signal
91 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current Sensor 1
92 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal Sensor 1
93-94 | -- | -- | Not Used
95 | 0.5 GY | 597 | 5-Volt Reference 1
96 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control Sensor 1

### Engine Control Module (ECM) X2

#### Connector Part Information

- OEM: 1 928 404 916
- Description: 58-Way F Sealed (BK)

#### Engine Control Module (ECM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 BK/WH | 451 | Ground
2 | 2.0 BK/WH | 451 | Ground
3 | 0.8 PK/BK | 5290 | Ignition 1 Voltage
4 | 1.0 BK/WH | 451 | Ground
5 | 0.8 PK/BK | 5290 | Ignition 1 Voltage
6 | 0.8 PK/BK | 5290 | Ignition 1 Voltage
7 | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control Sensor 2
8 | -- | -- | Not Used
9 | 0.5 TN | 2759 | Low Reference
10 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
11 | 0.35 TN | 5514 | Low Reference
12 | -- | -- | Not Used
13 | 0.35 YE | 492 | Mass Air Flow Sensor Signal
14 | 0.5 GY | 2709 | 5-Volt Reference 1
15 | 0.35 D-BU | 1161 | Throttle Position Sensor 1 Signal
16 - 17 | -- | -- | Not Used
18 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage (MA5)
19 | 0.5 WH | 1310 | EvaporativeEmission Canister Vent Solenoid Control
20 | 0.5 BN | 7448 | Vacuum Assist Pump Relay Coil Control (Late Production)
21 | -- | -- | Not Used
22 | 0.35 TN | 2760 | Low Reference
23 | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal Sensor 2
24 | -- | -- | Not Used
25 | 0.35 L-BU | 1162 | Throttle Position Sensor 2 Signal
26 | -- | -- | Not Used
27 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
28 | -- | -- | Not Used
29 | 0.5 OG | 6030 | Brake Booster Vacuum Sensor Signal (Late Production)
30 - 33 | -- | -- | Not Used
34 | 0.35 BN | 1271 | Low Reference
35 | 0.35 GY | 2700 | 5-Volt Reference 3
36 | 0.5 PU | 1589 | Fuel Level Sensor Signal
37 | 0.35 L-GN | 6338 | Manual Transmission Clutch Position Sensor Signal Position (MA5)
38 | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal Sensor 2
39 | 0.5 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal (C60)
40 | 0.5 PU | 401 | Vehicle Speed Sensor Low Signal (MA5)
41 | 0.35 BN | 4 | Accessory Voltage
42 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
43 | -- | -- | Not Used
44 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control (C60)
45 | -- | -- | Not Used
46 | 0.35 WH | 2368 | Cooling Fan Speed Control
47 | 0.35 PU | 1272 | Low Reference
48 | 0.35 TN | 1274 | 5-Volt Reference 3
49 | 0.35 WH/BK | 1164 | 5-Volt Reference 2
50 | 0.35 L-BU | 6289 | Induction Air Temperature Sensor Signal
51 | -- | -- | Not Used
52 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage (MA5)
53 | 0.5 YE | 400 | Vehicle Speed Sensor High Signal (MA5)
54 | 0.5 PK | 1039 | Ignition 1 Voltage
55 | 0.5 TN | 2501 | High Speed GMLAN Serial Data BUS (-)
56 | 0.5 RD/WH | 840 | Battery Positive Voltage
57 | 0.35 PU/WH | 6386 | Starter Enable Relay (PPEI 3) Control
58 | 0.35 YE | 5991 | Powertrain Relay Control

### Engine Coolant Level Switch

#### Connector Part Information

- OEM: 12052641
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Engine Coolant Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN | 1478 | Coolant Level Switch Signal
B | 0.5 BK/WH | 451 | Ground

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 15449028
- Description: 2-Way F GT 150 Sealed (BK)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 2761 | Low Reference
B | 0.5 YE | 410 | ECT Sensor Signal

### Engine Cooling Fan

#### Connector Part Information

- OEM: 7283-8496-30
- Description: 4-Way F Mixed Series, Sealed (BK)

#### Engine Cooling Fan

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 8.0 RD/BK | 342 | Battery Positive Voltage
2 | 8.0 BK | 650 | Ground
3 | -- | -- | Not Available
4 | 0.35 WH | 2368 | Cooling Fan Speed Control

### Engine Oil Pressure (EOP) Switch

#### Connector Part Information

- OEM: 15474881
- Description: 4-Way F Metri-Pack 150 Series Sealed (GY)

#### Engine Oil Pressure (EOP) Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
B-D | -- | -- | Not Used

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage
B | 0.5 D-GN/WH | 428 | Evaporative Emission Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 140 | Battery Positive Voltage
B | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control

### Evaporator Temperature Sensor (C60)

#### Connector Part Information

- OEM: 12047662
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Evaporator Temperature Sensor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 1791 | Low Reference
B | 0.35 GY | 6137 | Evaporator Core Temperature Sensor Signal

### Fog Lamp - Left Front (T96)

#### Connector Part Information

- OEM: 12124819
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Fog Lamp - Left Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 2234 | Front Fog Lamp Supply Voltage
B | 0.5 BK | 150 | Ground

### Fog Lamp - Rear (T79)

#### Connector Part Information

- OEM: 6189-0264
- Description: 2-Way F 090 Series Sealed (L-GY)

#### Fog Lamp - Rear (T79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage
2 | 0.5 BK | 750 | Ground

### Fog Lamp - Right Front (T96)

#### Connector Part Information

- OEM: 12124819
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Fog Lamp - Right Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 2234 | Front Fog Lamp Supply Voltage
B | 0.5 BK | 250 | Ground

### Fog Lamp Switch - Front (T96)

#### Connector Part Information

- OEM: 15419483
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Fog Lamp Switch - Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 550 | Ground
B | 0.35 YE | 317 | Fog Lamp Relay Control
C | 0.35 OG | 192 | Front Fog Lamp Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage

### Fog Lamp Switch - Rear (T79)

#### Connector Part Information

- OEM: 12047785
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Fog Lamp Switch - Rear (T79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 550 | Ground
B | -- | -- | Not Used
C | 0.35 L-BU | 187 | Rear Fog Lamp Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage

### Folding Top Cover Actuator

#### Connector Part Information

- OEM: 15326870
- Description: 2-Way FGT 280 (BK)

#### Folding Top Cover Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 TN/WH | 56 | Trunk Release Motor Supply Voltage
B | 1.0 BK | 850 | Ground

### Fuel Injector 1

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 1.0 TN | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1

### Fuel Injector 2

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
2 | 1.0 TN | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2

### Fuel Injector 3

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
2 | 1.0 TN | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3

### Fuel Injector 4

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Fuel Injector 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
2 | 1.0 TN | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 15326631
- Description: 4-Way F GT 280 Series Sealed (BK)

#### Fuel Pump and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 750 | Ground
B | 0.5 PU | 1589 | Fuel Level Sensor Signal
C | 0.5 TN | 2759 | Low Reference
D | 1.0 GY | 120 | Fuel Pump Supply Voltage

### Fuel Rail Pressure (FRP) Sensor

#### Connector Part Information

- OEM: 1 928 403 966
- Description: 3-Way F 2.8 Series Sealed (BK)

#### Fuel Rail Pressure (FRP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 808 | Low Reference
2 | 0.5 GY | 2918 | Fuel Rail Pressure Sensor Signal
3 | 0.5 GY | 598 | 5-Volt Reference 1

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 13511996
- Description: 3-Way F GT 150 Series, Sealed (GY)

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.5 TN | 2759 | Low Reference
3 | 0.5 GY | 2709 | 5-Volt Reference 1

### Generator X1

#### Connector Part Information

- OEM: 12186568
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Generator X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 OG | 225 | Generator Turn On Signal
C | 0.35 GY | 23 | Generator Field Duty Cycle Signal
D | -- | -- | Not Used

### Generator X2

#### Terminal Part Information

- Terminal: 12146365
- Description: Ring Terminal

#### Generator X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 13 RD | 2 | Battery Positive Voltage

### Hazard Warning Switch

#### Connector Part Information

- OEM: 12047781
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Hazard Warning Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
B | 0.35 BK | 550 | Ground
C | 0.35WH | 111 | Hazard Switch Signal

### Headlamp - Left High Beam

#### Connector Part Information

- OEM: 15393199
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Headlamp - Left High Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | -- | Left Headlamp High Beam Supply Voltage
B | 0.8 BK | -- | Ground

### Headlamp - Left Low Beam

#### Connector Part Information

- OEM: 15393199
- Description: 2-Way F Metri-Pack 280 Series Sealed (GY)

#### Headlamp - Left Low Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD | -- | Left Headlamp Low Beam Supply Voltage
B | 0.8 RD | -- | Ground

### Headlamp - Right High Beam

#### Connector Part Information

- OEM: 15393199
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Headlamp - Right High Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | -- | Right Headlamp High Beam Supply Voltage
B | 0.8 BK | -- | Ground

### Headlamp - Right Low Beam

#### Connector Part Information

- OEM: 15393199
- Description: 2-Way F Metri-Pack 280 Series Sealed (GY)

#### Headlamp - Right Low Beam

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD | -- | Right Headlamp Low Beam Supply Voltage
B | 0.8 RD | -- | Ground

### Heated Oxygen Sensor (HO2S) 1

#### Connector Part Information

- OEM: 1 928 404 900
- Description: 6-Way F Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH | 5279 | Heated Oxygen Sensor Pump Current - Sensor 1
2 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal - Sensor 1
3 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control - Sensor 1
4 | 0.5 PK/BK | 5291 | Ignition 1 Voltage
5 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current - Sensor 1
6 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal - Sensor 1

### Heated Oxygen Sensor (HO2S) 2

#### Connector Part Information

- OEM: 15326423
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal - Sensor 2
B | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal - Sensor 2
C | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control - Sensor 2
D | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### High Pressure Fuel Pump

#### Connector Part Information

- OEM: 1 928 403 874
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### High Pressure Fuel Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
2 | 1.0 YE | 7301 | High Pressure Fuel Pump Actuator High Control

### Horn - Left

#### Connector Part Information

- OEM: E-2157-000
- Description: 2-Way F Sleeve Assembly Wire Connector (BK)

#### Horn - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK | 150 | Ground
2 | 0.8 D-GN | 29 | Horn Control

### Horn - Right

#### Connector Part Information

- OEM: E-2157-000
- Description: 2-Way F Sleeve Assembly Wire Connector (BK)

#### Horn - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK | 250 | Ground
2 | 0.8 D-GN | 29 | Horn Control

### Horn Switch

#### Connector Part Information

- OEM: 1209251
- Description: 2-Way F (RD)

#### Horn Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BN | 28 | Horn Relay Control
B | 0.35 BK/WH | 1150 | Ground
0.35 BK/WH | 1150 | Ground

### HVAC Control Module X1

#### Connector Part Information

- OEM: 1534390-1
- Description: 5-Way F (BK)

#### HVAC Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 OG | 52 | Blower Motor High Control
2 | 2.0 L-BU | 72 | Medium 2 Blower Motor Control
3 | 2.0 TN | 63 | Blower Motor Medium Control (1)
4 | 2.0 YE | 60 | Blower Motor Low Control
5 | 2.0 BK | 550 | Ground

### HVAC Control Module X2

#### Connector Part Information

- OEM: 15336594
- Description: 12-Way F Micro-Pack 100 Series (GY)

#### HVAC Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 RD/WH | 1540 | Battery Positive Voltage
C | 0.35 BK | 550 | Ground
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
E | -- | -- | Not Used
F | 0.35 WH | 193 | Rear Defog Relay Control
G | 0.35 D-GN/WH | 762 | A/C Request Signal (C60)
H | -- | -- | Not Used
J | 0.35 L-BU | 292 | Rear Defog Switch Signal
K | 0.5 PK | 339 | Ignition 1 Voltage
L | 0.35 BK/WH | 651 | Ground
M | -- | -- | Not Used

### HVAC Control Module X3

#### Connector Part Information

- OEM: 12064799
- Description: 12-Way F Micro-Pack 100 Series (BK)

#### HVAC Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 1791 | Low Reference
B | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal
C | 0.35 GY | 6137 | Evaporator Core Temperature Sensor Signal (C60)
D | 0.35 D-BU | 1646 | Air Temperature Door Position Signal
E | 0.35 L-BU | 733 | Air Temperature Door Position Signal
F | 0.35 L-BU/BK | 1688 | 5-Volt Reference
G | 0.35 D-GN | 1614 | Recirculation Door Control
H | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit
J | 0.35 L-GN | 2275 | Mode Door Control
K | 0.35 TN | 2273 | Mode Door Control
L | 0.35 L-GN/BK | 1647 | Air Temperature Door Control
M | 0.35 D-BU | 1199 | Air Temperature Door Control

### I/P Dimmer Switch

#### Connector Part Information

- OEM: 12020299
- Description: 5-Way F P/C Edgeboard - Standard (NA)

#### I/P Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 PU | 719 | Low Reference
C | 0.35 D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal
D-E | -- | -- | Not Used

### Ignition Coil 1

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN | 2129 | Low Reference
3 | 0.35 PU | 2121 | IC 1 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 2

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN/WH | 2130 | Low Reference
3 | 0.35 OG/WH | 2122 | IC 2 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 3

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN | 2129 | Low Reference
3 | 0.35 L-BU | 2123 | IC 3 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil 4

#### Connector Part Information

- OEM: 7283-3392-30
- Description: 4-Way F GT 150 Series (BK)

#### Ignition Coil 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 450 | Ground
2 | 0.35 BN/WH | 2130 | Low Reference
3 | 0.35 D-GN/WH | 2124 | IC 4 Control
4 | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Switch

#### Connector Part Information

- OEM: 1L-AG5-6S-S3C1
- Description: 6-Way F 1L - AG5 Series (GN)

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 RD/WH | 1040 | Battery Positive Voltage
3 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
4 | 0.35 BN | 4 | Accessory Voltage
5 | 0.35 WH | 1390 | Off/Run/Crank Voltage
6 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal

### Inflatable Restraint Front End Sensor - Left

#### Connector Part Information

- OEM: PE075692
- Description: 2-Way F GT 150 Series Sealed 4.0 (YE)

#### Inflatable Restraint Front End Sensor - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/OG | 5045 | Low Reference
B | 0.5 YE | 1834 | Forward Discriminating Sensor Signal

### Inflatable Restraint Front End Sensor - Right

#### Connector Part Information

- OEM: PE075692
- Description: 2-Way F GT 150 Series Sealed 4.0 (YE)

#### Inflatable Restraint Front End Sensor - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 5600 | Low Reference
B | 0.5 YE/BK | 2160 | Front End Discriminating Sensor Signal

### Inflatable Restraint I/P Module X1

#### Connector Part Information

- OEM: 54550268
- Description: 2-Way F (GY) With (YE) Case

#### Inflatable Restraint I/P Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 3024 | Instrument Panel Module - Stage 1 - Low Control
2 | 0.5 L-BU/RD | 3025 | Instrument Panel Module - Stage 1 - High Control

### Inflatable Restraint I/P Module X2

#### Connector Part Information

- OEM: 54550266
- Description: 2-Way F (BK) With (YE) Case

#### Inflatable Restraint I/P Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN/RD | 3026 | Instrument Panel Module - Stage 2 - Low Control
2 | 0.5 RD/WH | 3027 | Instrument Panel Module - Stage 2 - High Control

### Inflatable Restraint I/P Module Indicator

#### Connector Part Information

- OEM: 15398877
- Description: 5-Way F HCM (WH)

#### Inflatable Restraint I/P Module Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/BK | 723 | Instrument Panel Module Disable Switch Signal
2 | 0.35 BK/WH | 651 | Ground
3 | 0.35 PK | 353 | Instrument Panel Module Suppression Indicator Control
4 | 0.5 PK | 339 | Ignition 1 Voltage
5 | 0.35 PU | 5234 | Passenger Seat Belt Indicator

### Inflatable Restraint Passenger Presense System (PPS) Module

#### Connector Part Information

- OEM: 15332142
- Description: 6-Way M GT 150 Series (BK)

#### Inflatable Restraint Passenger Presense System (PPS) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 1339 | Ignition 1 Voltage
B | 0.35 PK | 5018 | Occupant Sensor Serial Data
C | 0.35 TN | 723 | Instrument Panel Module Disable Switch Signal
D | 0.35 BK/WH | 351 | Ground
E | 0.35 PK | 353 | Instrument Panel Module Suppression Indicator Control
F | -- | -- | Not Used

### Inflatable Restraint Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: 6-638595-2
- Description: 60-Way F (YE)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1240 | Battery Positive Voltage
2 | 0.35 D-GN/YE | 5060 | Low Speed GMLAN Serial Data
3 | 0.35 PK | 5057 | Low Reference
4 | 0.35 TN/WH | 238 | Seat Belt Switch - Driver
5 | -- | -- | Not Used
6 | 0.35 OG | 1362 | Seat Belt Switch - Signal - Passenger
7 | -- | -- | Not Used
8-11 | -- | -- | Not Available
12 | 0.5 PU | 3026 | Instrument Panel Module Stage 2 Low Control
13 | 0.5 GY | 3027 | Instrument Panel Module Stage 2 High Control
14 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 High Control
15 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 Low Control
16 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 Low Control
17 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 High Control
18 | 0.5 YE | 3025 | Instrument Panel Module - Stage 1 High Control
19 | 0.5 OG | 3024 | Instrument Panel Module - Stage 1 Low Control
20-30 | -- | -- | Not Available
31 | 0.5 BK/WH | 351 | Ground
32 | -- | -- | Not Available
33 | 0.35 PK | 1339 | Ignition 1 Voltage
34-35 | -- | -- | Not Available
36 | 0.5 GY | 5600 | Front End Sensor - Voltage - Right
37 | 0.5 YE/BK | 2160 | Front End Sensor - Signal - Right
38 | 0.5 YE | 1834 | Front End Sensor - Voltage - Left
39 | 0.5 TN/OG | 5045 | Front End Sensor - Signal - Left
40-51 | -- | -- | Not Available
52 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Passenger - High Control
53 | 0.5 OG | 2117 | Seat Belt Pretensioner - Passenger - Low Control
54-55 | -- | -- | Not Available
56 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Driver - High Control
57 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Driver - Low Control
58-59 | -- | -- | Not Available
60 | 0.35 PK | 5018 | Occupant Sensor Serial Data

### Inflatable Restraint Steering Wheel Module X1

#### Connector Part Information

- OEM: 15359118
- Description: 2-Way F Micro-Pack 100 Series (GY) With (WH) Case

#### Inflatable Restraint Steering Wheel Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
B | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control

### Inflatable Restraint Steering Wheel Module X2

#### Connector Part Information

- OEM: 15359118
- Description: 2-Way F Micro-Pack 100 Series (GY) With (PK) Case

#### Inflatable Restraint Steering Wheel Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
B | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15393433
- Description: 10-Way F Micro-Pack 064 Series Unsealed (BK)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PK | 1539 | Ignition 1 Voltage
D | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 WH/BK | 644 | 10-Volt Reference
G | 0.35 GY | 1458 | Instrument Panel Lamp Supply Voltage (UK3)
H | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
J | 0.35 BN | 28 | Horn Relay Control
K | 0.35 BK | 1150 | Ground

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15393433
- Description: 10-Way F Micro-Pack 064 Series Unsealed (BK)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PK | 1539 | Ignition 1 Voltage
D | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 WH/BK | 644 | 10-Volt Reference (UK3)
G | 0.35 GY/BK | 1458 | Instrument Panel Lamp Supply Voltage - 4
H | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
J | 0.35 TN | 28 | Horn Relay Control
K | 0.5 BK | 1150 | Ground

### Inflatable Restraint Steering Wheel Module Coil X3

#### Connector Part Information

- OEM: 15393421
- Description: 4-Way F Micro-Pack 064 (YE)

#### Inflatable Restraint Steering Wheel Module Coil X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
2 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
3 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
4 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 High Control

### Inside Rearview Mirror (ISRVM)

#### Connector Part Information

- OEM: 12124782
- Description: 7-Way F VH Series (BK)

#### Inside Rearview Mirror (ISRVM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BK | 550 | Ground
3-5 | -- | -- | Not Used
6 | 0.5 GY | 157 | Courtesy Lamp Control
7 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 15429805
- Description: 16-Way F (NA)

#### Instrument Panel Cluster (IPC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
6 | 0.35 BN/WH | 419 | MIL Control
7 | -- | -- | Not Used
8 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
9 | 0.35 D-GN/BK | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.35 PK | 339 | Ignition 1 Voltage
12 | -- | -- | Not Used
13 | 0.35 RD/WH | 1440 | Battery Positive Voltage
14 | 0.35 D-GN | 264 | Security Indicator Supply Voltage
15 | 0.5 BK/WH | 1150 | Ground
16 | 0.35 BK | 550 | Ground

### Intake Air Pressure and Temperature Sensor

#### Connector Part Information

- OEM: 12162187
- Description: 4-Way F Metri-Pack 150.2 Series Sealed, Pull to Seat (BK)

#### Intake Air Pressure and Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 407 | Low Reference
B | 0.5 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
C | 0.5 GY | 597 | 5-Volt Reference 1
D | 0.5 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal

### Knock Sensor (KS) - 1

#### Connector Part Information

- OEM: 12077900
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Knock Sensor (KS) - 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 496 | Knock Sensor 1 Signal
B | 0.5 GY | 1716 | Knock Sensor 1 Signal

### Knock Sensor (KS) - 2

#### Connector Part Information

- OEM: 12077900
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Knock Sensor (KS) - 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
B | 0.5 GY | 2303 | Knock Sensor 2 Signal

### License Lamp - Left

#### Connector Part Information

- OEM: 1452680-1
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### License Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 750 | Tail/License Lamps Supply Voltage
2 | 0.5 BN | 9 | Tail/License Lamps Supply Voltage

### License Lamp - Right

#### Connector Part Information

- OEM: 1452680-1
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### License Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 750 | Tail/License Lamps Supply Voltage
2 | 0.5 BN | 9 | Tail/License Lamps Supply Voltage

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: 184032-1
- Description: 3-Way F SSC Sealed Series (BK)

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 597 | 5-Volt Reference 1
2 | 0.5 TN | 407 | Low Reference
3 | 0.5 L-GN | 432 | Manifold Absolute Pressure Sensor Signal

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 15326822
- Description: 5-Way F GT 150 Series Sealed (BK)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 492 | Mass Air Flow Sensor Signal
B | 0.35 BK/WH | 451 | Ground
C | 0.35 PK/BK | 5291 | Ignition 1 Voltage
D | 0.35 TN | 2760 | Low Reference
E | 0.35 L-BU | 6289 | Induction Air Temperature Sensor Signal

### Mode Actuator

#### Connector Part Information

- OEM: 12064982
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Mode Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 1791 | Low Reference
2 | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal
3 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
4 | 0.35 TN | 2273 | Mode Door Control
5 | 0.35 L-GN | 2275 | Mode Door Control

### Outside Air Temperature Sensor

#### Connector Part Information

- OEM: 12052642
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GN)

#### Outside Air Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN/WH | 636 | Ambient Air TemperatureSensor Signal
B | 0.5 YE | 61 | Low Reference

### Outside Rearview Mirror - Driver (D48)

#### Connector Part Information

- OEM: E-5965-003
- Description: 3-Way M 1.5 Series Sealed (BK)

#### Outside Rearview Mirror - Driver (D48)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 81 | Driver Mirror Motor Left Control
2 | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
3 | 0.35 L-GN | 89 | Driver Mirror Motor Up Control

### Outside Rearview Mirror - Passenger (D48)

#### Connector Part Information

- OEM: E-5965-003
- Description: 3-Way M 1.5 Series Sealed (BK)

#### Outside Rearview Mirror - Passenger (D48)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control
2 | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
3 | 0.35 PU/WH | 889 | Passenger Mirror Motor Up Control

### Outside Rearview Mirror Switch (D48)

#### Connector Part Information

- OEM: 12064769
- Description: 10-Way F Metri-Pack 150 Series (NA)

#### Outside Rearview Mirror Switch (D48)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK | 550 | Ground
C | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
D | 0.35WH | 81 | Driver Mirror Motor Right Control
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
F | 0.35 L-GN | 89 | Driver Mirror Motor Down Control
G | 0.35 RD/WH | 440 | Battery Positive Voltage
H | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
J | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control
K | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control

### Park Brake Switch

#### Connector Part Information

- OEM: 12047682
- Description: 1-Way F Metri-Pack 150 Series (BK)

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1134 | Park Brake Switch Signal

### Park Lamp - Left Front

#### Connector Part Information

- OEM: E-3550-000
- Description: 2-Way F 1.5 Series Sealed (BK)

#### Park Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Supply Voltage
2 | 0.8 BK | 250 | Ground

### Park Lamp - Right Front

#### Connector Part Information

- OEM: E-3550-000
- Description: 2-Way F 1.5 Series Sealed (BK)

#### Park Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Supply Voltage
2 | 0.8 BK | 150 | Ground

### Radio - X1

#### Connector Part Information

- OEM: 7283-9076-30
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Radio - X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 PK | 314 | Radio On Signal (UQ3)
4 | 0.5 L-BU | 115 | Right Rear Speaker Output (-) (UW5)
0.5 TN | 1946 | Right Rear Low Level Audio Signal (-) (UQ3)
5 | 0.5 D-BU | 46 | Right Rear Speaker Output (+) (UW5)
0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+) (UQ3)
6 | 0.5 YE | 116 | Left Rear Speaker Output (-) (UW5)
0.5 BN | 1999 | Left Rear Low Level Audio Signal (-) (UQ3)
7 | 0.5 BN | 199 | Left Rear Speaker Output (+) (UW5)
0.5 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (UQ3)
8-13 | -- | -- | Not Used
14 | 0.35 WH/BK | 644 | 10-Volt Reference (UK3)
15 | 0.35 L-GN | 1011 | Remote Radio Control Signal (UQ3)
16 | -- | -- | Not Used

### Radio - X2

#### Connector Part Information

- OEM: 7283-4490-30
- Description: 14-Way F (BK)

#### Radio - X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 RD/WH | 1140 | Battery Positive Voltage
2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
3 | -- | -- | Not Used
4 | 0.5 D-GN | 117 | Right Front Speaker Output (-) (UW5)
0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-) (UQ3)
5 | 0.5 L-GN | 200 | Right Front Speaker Output (+) (UW5)
0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+) (UQ3)
6 | 0.5 GY | 118 | Left Front Speaker Output (-) (UW5)
0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-) (UQ3)
7 | 0.5 TN | 201 | Left Front Speaker Output (+) (UW5)
0.5 TN | 511 | Left Front Low Level Audio Signal (+) (UQ3)
8 | 0.8 BK/WH | 551 | Ground
9 | 0.35 D-GN/WH | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.35 D-BU | 1796 | Steering Column Controls Signal
12-14 | -- | -- | Not Used

### Rear Compartment Courtesy Lamp

#### Connector Part Information

- OEM: 12047662
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Rear Compartment Courtesy Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 750 | Ground
B | 0.5 OG/BK | 737 | Rear Compartment Lamp Control

### Rear Compartment Lid Ajar Switch

#### Connector Part Information

- OEM: 12129082
- Description: 2-Way F Metri-Pack 280 Series Flexlock (GY)

#### Rear Compartment Lid Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
B | 0.5 BK | 850 | Ground

### Rear Compartment Lid Release Actuator

#### Connector Part Information

- OEM: 12129081
- Description: 2-Way F Metri-Pack 280 Series Flexlock (BK)

#### Rear Compartment Lid Release Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 TN/WH | 56 | Rear Compartment Lid Release Motor Supply Voltage
B | 1.0 BK | 850 | Ground

### Rear Compartment Lid Release Switch

#### Connector Part Information

- OEM: 12044785
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Rear Compartment Lid Release Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 651 | Ground
B | -- | -- | Not Used
C | 0.35 TN | 1576 | Rear Compartment Lid Release Actuator
D | -- | -- | Not Used

### Rear Window Defogger Grid X1

#### Connector Part Information

- OEM: 12004267
- Description: 1-Way F 56 Series Lock Type (BK)

#### Rear Window Defogger Grid X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 293 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid X2

#### Connector Part Information

- OEM: 12004267
- Description: 1-Way F 56 Series Lock Type (BK)

#### Rear Window Defogger Grid X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 BK | 850 | Ground

### Recirculation Actuator

#### Connector Part Information

- OEM: 12064982
- Description: 5-Way F Micro-Pack 100 Series (BK)

#### Recirculation Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | 0.35 D-GN | 1614 | Recirculation Door Control
5 | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit

### Remote Control Door Lock Receiver (RCDLR) (AU3/AU0)

#### Connector Part Information

- OEM: HCMPB-04-K
- Description: 4-Way F HCM Series (BK)

#### Remote Control Door Lock Receiver (RCDLR) (AU3/AU0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 851 | Ground
2 | 0.35 D-GN/RD | 5060 | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | 0.35 RD/WH | 1340 | Battery Positive Voltage

### Seat Adjuster Switch - Driver (AF2)

#### Connector Part Information

- OEM: 12052854
- Description: 7-Way F Metri-Pack 280 Series (BK)

#### Seat Adjuster Switch - Driver (AF2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2.0 BK | 550 | Ground
B | 2.0 D-BU | 287 | Driver Seat Front Vertical Motor Down Control
C | 2.0 D-GN | 286 | Driver Seat Front Vertical Motor Up Control
D-E | -- | -- | Not Used
F | 2.0 RD/BK | 642 | Battery Positive Voltage
G | 2.0 BK | 550 | Ground

### Seat Belt Pretensioner - Driver

#### Connector Part Information

- OEM: 15380395
- Description: 2-Way F Squib Unsealed (YE)

#### Seat Belt Pretensioner - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Driver - Low Control
2 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Driver - High Control

### Seat Belt Pretensioner - Passenger

#### Connector Part Information

- OEM: 15380395
- Description: 2-Way F Squib Unsealed (YE)

#### Seat Belt Pretensioner - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 2117 | Seat Belt Pretensioner - Passenger - Low Control
2 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Passenger - High Control

### Seat Belt Switch - Driver

#### Connector Part Information

- OEM: 15332132
- Description: 3-Way F GT 150 Series (BK)

#### Seat Belt Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/WH | 238 | Seat Belt Switch Signal - Driver
B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference

### Seat Belt Switch - Passenger

#### Connector Part Information

- OEM: 15332133
- Description: 3-Way F GT 150 Series (BK)

#### Seat Belt Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1362 | Seat Belt Switch Signal - Passenger
B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference

### Seat Front Vertical Motor - Driver (AF2)

#### Connector Part Information

- OEM: 1379217-3
- Description: 5-Way F MQS/MPQ Mixed Series (BK)

#### Seat Front Vertical Motor - Driver (AF2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2.0 D-GN | 286 | Driver Seat Front Vertical Motor Up Control
2-4 | -- | -- | Not Used
5 | 2.0 D-BU | 287 | Driver Seat Front Vertical Motor Down Control

### Speaker - Left Front (UQ3)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Left Front (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-)
B | 0.8 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Front (UW5)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Left Front (UW5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-)
B | 0.8 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Rear (UQ3)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Left Rear (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 YE | 116 | Left Rear Speaker Output (-)
B | 0.8 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Left Rear (UW5)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Left Rear (UW5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 116 | Left Rear Speaker Output (-)
B | 0.5 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Left Tweeter

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Left Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 TN | 1856 | Left Tweeter Speaker Output (+) (UQ3)
0.8 GY | 118 | Left Front Speaker Output (-) (UW5)
B | 0.8 YE | 1956 | Left Tweeter Speaker Output (-) (UQ3)
0.8 TN | 201 | Left Front Speaker Output (+) (UW5)

### Speaker - Right Front (UQ3)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Right Front (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-GN | 117 | Right Front Speaker Output (-)
B | 0.8 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Front (UW5)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Right Front (UW5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-GN | 117 | Right Front Speaker Output (-)
B | 0.8 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Rear (UQ3)

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Right Rear (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 115 | Right Rear Speaker Output (-)
B | 0.8 D-BU | 46 | Right Rear Speaker Output (+)

### Speaker - Right Rear (UW5)

#### Connector Part Information

- OEM: 12064869
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Speaker - Right Rear (UW5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 115 | Right Rear Speaker Output (-)
B | 0.5 D-BU | 46 | Right Rear Speaker Output (+)

### Speaker - Right Tweeter

#### Connector Part Information

- OEM: 12052832
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Speaker - Right Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-GN | 1852 | Right Tweeter Speaker Output (+) (UQ3)
0.8 D-GN | 117 | Right Front Speaker Output (-) (UW5)
B | 0.8 PU | 1952 | Right Tweeter Speaker Output (-) (UQ3)
0.8 L-GN | 200 | Right Front Speaker Output (+) (UW5)

### Speaker - Subwoofer (UQ3)

#### Connector Part Information

- OEM: 12064760
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Speaker - Subwoofer (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-)
B | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+)
C | 0.8 L-GN/BK | 1794 | Left Subwoofer Speaker Output (-)
D | 0.8 D-BU/WH | 346 | Left Subwoofer Speaker Output (+)

### Starter Motor X1

#### Connector Part Information

- OEM: 12089916
- Description: 1-Way F Metri-Pack 280 Series, Sealed (BK)

#### Starter Motor X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2.0 PU | 6 | Starter Solenoid Crank Voltage

### Starter Motor X2

#### Terminal Part Information

- Terminal: 12103503
- Description: Ring Terminal

#### Starter Motor X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 5 RD | 2 | Starter Solenoid Crank Voltage

### Steering Angle Sensor (JL9)

#### Connector Part Information

- OEM: 1488752-1
- Description: 6-Way F 064 GET Series (BK)

#### Steering Angle Sensor (JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 2087 | 12-Volt Reference
2 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
3 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
4 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
5 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
6 | 0.5 L-BU | 2088 | Low Reference

### Steering Wheel Control Switch - Left (K34)

#### Connector Part Information

- OEM: 50-57-9407
- Description: 7-Way F SL Series Unsealed (BK)

#### Steering Wheel Control Switch - Left (K34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
2 | -- | -- | Not Used
3 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
4 | 0.35 PK | 1539 | Ignition 1 Voltage
5 | 0.35 GY | 1884 | Cruise Control Switch Signal
6 | -- | -- | Not Used
7 | 0.35 BK/WH | 1150 | Ground

### Steering Wheel Control Switch - Right (UK3)

#### Connector Part Information

- OEM: 50-57-9404
- Description: 4-Way F SL Series Unsealed (BK)

#### Steering Wheel Control Switch - Right (UK3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 1150 | Ground
2 | 0.35 WH/BK | 644 | 10-Volt Reference
3 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
4 | 0.35 D-BU | 1796 | Steering Column Controls Signal

### Tail/Stop Lamp - Left

#### Connector Part Information

- OEM: 6189-0319
- Description: 6-Way F TS 090 Series, Sealed (L-GY)

#### Tail/Stop Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 YE | 618 | Left Rear Turn Signal Lamp Supply Voltage
3 | 0.8 D-BU | 809 | Tail/License Lamps Supply Voltage
4 | -- | -- | Not Used
5 | 0.8 BK | 1050 | Ground
6 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage

### Tail/Stop Lamp - Right

#### Connector Part Information

- OEM: 6189-0319
- Description: 6-Way F TS 090 Series, Sealed (L-GY)

#### Tail/Stop Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 D-GN | 619 | Right Rear Turn Signal Lamp Supply Voltage
3 | 0.8 WH | 750 | Tail/License Lamps Supply Voltage
4 | -- | -- | Not Used
5 | 0.8 BK | 750 | Ground
6 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage

### Theft Deterrent Module (TDM)

#### Connector Part Information

- OEM: 50-57-9705
- Description: 5-Way F Sl Series Unsealed (BK)

#### Theft Deterrent Module (TDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1540 | Battery Positive Voltage
2 | 0.35 BN | 4 | Accessory Voltage
3 | 0.35 BK/WH | 651 | Ground
4 | 0.35 L-GN | 5060 | Low Speed GMLAN Serial Data
5 | -- | -- | Not Used

### Throttle Body

#### Connector Part Information

- OEM: 15355297
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Throttle Body

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 582 | Throttle Actuator Control Motor Control - 2
B | 0.8 YE | 581 | Throttle Actuator Control Motor Control - 1
C | 0.5 TN | 2752 | Low Reference
D | 0.5 D-GN | 485 | Throttle Position Sensor 1 Signal
E | 0.5 GY | 2701 | 5-Volt Reference 3
F | 0.5 PU | 486 | Throttle Position Sensor 2 Signal

### Traction Control Switch (TCS) (JL9)

#### Connector Part Information

- OEM: 12047785
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Traction Control Switch (TCS) (JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 550 | Ground
B | -- | -- | Not Used
C | 0.35 L-BU | 1788 | Traction Control Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply

### Turbocharger Bypass Valve Solenoid

#### Connector Part Information

- OEM: 1 928 402 571
- Description: 2-Way F Sealed (BK)

#### Turbocharger Bypass Valve Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 6391 | Turbocharger Bypass Valve Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turbocharger Wastegate Solenoid

#### Connector Part Information

- OEM: 1 928 402 571
- Description: 2-Way F Sealed (BK)

#### Turbocharger Wastegate Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 258 | Wastegate Solenoid Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turn Signal Lamp - Left Front

#### Connector Part Information

- OEM: 7822-2540-A44
- Description: 3-Way F (BK)

#### Turn Signal Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
MAJOR | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
MINOR | 0.5 BN | 9 | Park Lamp Supply Voltage
GRND | 0.5 BK | 150 | Ground

### Turn Signal Lamp - Right Front

#### Connector Part Information

- OEM: 7822-2540-A44
- Description: 3-Way F (BK)

#### Turn Signal Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
mAJOR | 0.5 L-BU | 15 | Right Turn Signal Lamps Supply Voltage
MINOR | 0.5 BN | 9 | Park Lamp Supply Voltage
GRND | 0.5 BK | 250 | Ground

### Turn Signal Lamp - Left Rear

#### Connector Part Information

- OEM: 7822-2540-A44
- Description: 2-Way F (BK)

#### Turn Signal Lamp - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-GN | 618 | Left Rear Stop/Turn Lamp Supply Voltage
G | 0.8 BK | 1050 | Ground
0.8 BK | 1050 | Ground

### Turn Signal Lamp - Right Rear

#### Connector Part Information

- OEM: 7822-2540-A44
- Description: 2-Way F (BK)

#### Turn Signal Lamp - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 619 | Right Rear Stop/Turn Lamp Supply Voltage
G | 0.5 BK | 750 | Ground
0.5 BK | 750 | Ground

### Turn Signal Repeater - Left

#### Connector Part Information

- OEM: 15326806
- Description: 2-Way M 150 Series Sealed (BK)

#### Turn Signal Repeater - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
B | 0.5 BK | 150 | Ground

### Turn Signal Repeater - Right

#### Connector Part Information

- OEM: 15326806
- Description: 2-Way M 150 Series Sealed (BK)

#### Turn Signal Repeater - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 15 | Right Turn Signal Lamps Supply Voltage
B | 0.5 BK | 250 | Ground

### Turn Signal/Multifunction Switch X1

#### Connector Part Information

- OEM: NACP-08-S
- Description: 8-Way F Misc (WH)

#### Turn Signal/Multifunction Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 651 | Ground
2 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
3 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
4 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
5-8 | -- | -- | Not Used

### Turn Signal/Multifunction Switch X2

#### Connector Part Information

- OEM: 15393435
- Description: 10-Way F Micro (BK)

#### Turn Signal/Multifunction Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK/WH | 651 | Ground
C | 0.35 BN | 1356 | Flash To Pass Switch Signal
D | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
E | -- | -- | Not Used
F | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control
G | 0.35 YE/BK | 1418 | Left Rear Turn Signal Switch Signal
H | 0.35 D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
J-K | -- | -- | Not Used

### Vehicle Speed Sensor (VSS) (MA5)

#### Connector Part Information

- OEM: 15336024
- Description: 2-Way F GT 150 Series Sealed Delphi Packard (BK)

#### Vehicle Speed Sensor (VSS) (MA5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 401 | Vehicle Speed Sensor Low Signal
B | YE | 400 | Vehicle Speed Sensor High Signal

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

- OEM: 1-928-403-698
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | 0.8 YE | 873 | Low Reference

### Wheel Speed Sensor (WSS) - Left Rear

#### Connector Part Information

- OEM: 13115612
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 TN | 884 | Left Rear Wheel Speed Sensor Signal
2 | 0.8 OG | 885 | Low Reference

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

- OEM: 1-928-403-698
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 D-GN | 872 | Right Front Wheel Speed Sensor Signal
2 | 0.8 TN | 833 | Low Reference

### Wheel Speed Sensor (WSS) - Right Rear

#### Connector Part Information

- OEM: 13115612
- Description: 2-Way Sealed F (BK)

#### Wheel Speed Sensor (WSS) - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal
2 | 0.8 WH | 883 | Low Reference

### Window Motor - Driver (A31)

#### Connector Part Information

- OEM: 12129487
- Description: 2-Way F Metri-Pack Series Flexlock Sealed (GY)

#### Window Motor - Driver (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 BN | 165 | Power Window Motor Left Front Down Control
B | 3.0 D-BU | 164 | Power Window Motor Left Front Up Control

### Window Motor - Passenger (A31)

#### Connector Part Information

- OEM: 12129487
- Description: 2-Way F Metri-Pack 280 Series FlexLock Sealed (GY)

#### Window Motor - Passenger (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 BN | 667 | Power Window Motor Right Front Down Control
B | 3.0 D-BU | 666 | Power Window Motor Right Front Up Control

### Window Switch - Driver (A31)

#### Connector Part Information

- OEM: 15449340
- Description: 8-Way F GT 280 (BK)

#### Window Switch - Driver (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 0.35 GY | 8 | Instrument Panel Lamp Supply
C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 2.0 BK | 550 | Ground
G | 3.0 D-BU | 164 | Power Window Motor Left Front Up Control
H | 3.0 BN | 165 | Power Window Motor Left Front Down Control

### Window Switch - Passenger (A31)

#### Connector Part Information

- OEM: 12192825
- Description: 8-Way F Metri-Pack 280 Series (BN)

#### Window Switch - Passenger (A31)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 0.35 BK | 550 | Ground
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 3.0 BN | 667 | Power Window Motor Right Front Down Control
G | 3.0 D-BU | 666 | Power Window Motor Right Front Up Control
H | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: 12052641
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Windshield Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 228 | Windshield Washer Pump Control
B | 0.5 BK | 250 | Ground

### Windshield Wiper Motor

#### Connector Part Information

- OEM: 15393432
- Description: 5-Way F 090 II Class III Series Sealed (BK)

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.0 BK | 250 | Ground
2 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
3 | -- | -- | Not Used
4 | 1.0 PU | 92 | Windshield Wiper Motor High Speed Control
5 | 1.0 D-GN | 95 | Windshield Washer Switch Signal

### Windshield Wiper/Washer Switch

#### Connector Part Information

- OEM: 12059800
- Description: 5-Way F Metri-Pack 150 Series (BK)

#### Windshield Wiper/Washer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 OG | 228 | Windshield Washer Pump Control
C | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
D | 0.35 PK | 439 | Ignition 1 Voltage
E | 0.35 GY | 112 | Windshield Wiper Switch Signal

### Yaw and Lateral Accelerometer Sensor (JL9)

#### Connector Part Information

- OEM: 2-967616-1
- Description: 6-Way F MQS Socket Series, Sealed (BK)

#### Yaw and Lateral Accelerometer Sensor (JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY/BK | 6435 | Can Bus Low Serial Data
2 | 0.5 PK/BK | 6434 | Can Bus High Serial Data
3 | 0.5 D-GN | 2087 | 12-Volt Reference
4 | -- | -- | Not Used
5 | 0.5 L-BU | 2088 | Low Reference
6 | -- | -- | Not Used