For 1990-2009 cars

Connector 1: | Clutch Pedal Position (CPP) Switch (MA5)
Connector 2: | Clutch Start Switch (MA5)
Connector 3: | Generator X1

### Clutch Pedal Position (CPP) Switch (MA5)

#### Connector Part Information

- OEM: 15479480
- Description: 2-Way F Micro-Pack 280 Series (L-GY)

#### Clutch Pedal Position (CPP) Switch (MA5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 BN/WH | 379 | CPP Switch Signal
B | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### Clutch Start Switch (MA5)

#### Connector Part Information

- OEM: 12041433
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Clutch Start Switch (MA5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 PK | 339 | Ignition 1 Voltage
B | 0.5 YE | 575 | Starter Contact Control

### Generator X1

#### Connector Part Information

- OEM: 12186568
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Generator X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 OG | 225 | Generator Turn On Signal
C | 0.35 GY | 23 | Generator Field Duty Cycle Signal
D | -- | -- | Not Used