For 1990-2009 cars

## Engine Support Fixture Rear Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine sight shield. Refer to Engine Sight Shield Replacement.

1 | Engine Support Fixture Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Engine Support Fixture

## Engine Support Fixture Front Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine sight shield. Refer to Engine Sight Shield Replacement.

1 | Engine Support Fixture Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18.4 lb ft)
2 | Engine Support Fixture