For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Rear Axle Lower Control Arm Fastener (GNC) | 70 N·m + 90 degrees+ 15 degrees | 51 lb ft+ 90 degrees+ 15 degrees
Rear Axle Lower Control Arm Fastener (GNE) | 115 N·m + 90 degrees+ 15 degrees | 85 lb ft+ 90 degrees+ 15 degrees
Rear Axel Upper Control Arm Inner Fastener | 150 N·m | 111 lb ft
Rear Axel Upper Control Arm Outer Fastener | 115 N·m | 85 lb ft + 90 degrees + 15 degees
Rear Suspension Link Inner Fastener (GNC) | 150 N·m | 111 lb ft
Rear Suspension Link Fastener | 150 N·m + 60 degrees + 15 degees | 111 lb ft + 60 degrees + 15 degees
Rear Suspension Link Outer Fastener | 115 N·m + 90 degrees + 15 degees | 85 lb ft + 90 degrees + 15 degees
Rear Suspension Link Outer Fastener | 150 N·m + 60 degrees + 15 degrees | 111 lb ft + 60 degrees + 15 degrees
Rear Wheel Hub Fastener | 90 N·m + 75 degrees | 66 lb ft + 75 degrees
Shock Absorber Lower Fastener (GNC) | 100 N·m + 75 degrees | 74 lb ft + 30 degrees
Shock Absorber Lower Fastener (GNE) | 110 N·m | 81 lb ft
Shock Absorber Upper Fastener (GNC) | 100 N·m + 75 degrees | 74 lb ft + 75 degrees
Shock Absorber Upper Fastener (GNE) | 150 N·m + 60 degrees + 15 degrees | 111 lb ft + 60 degrees + 15 degrees
Stabilizer Shaft Insulator Fastener | 22 N·m + 30 degrees | 16 lb ft + 30 degrees
Stabilizer Shaft Link Fastener | 50 N·m | 37 lb ft
Trailing Arm Fastener | 150 N·m + 30 degrees | 111 lb ft + 30 degrees