For 1990-2009 cars

The rear suspension system on this vehicle is of the independent link type. Rear suspension adjustment is achieved through adjustable toe links and lower control arms. The rear coil springs are retained between the body and the lower control arm. Rubber insulators isolate the coil spring at both top and bottom. The rear suspension consists of 2 shock absorbers attached to the knuckle and the reinforced body ares.

The rear suspension system performs the following functions:

• | Maintains the relationship of the rear axle to the body

• | Controls the torque reaction on acceleration and braking

The suspension system consists of the following components:

• | Support assembly

• | Coil springs and insulators

• | Stabilizer shaft, insulators and stabilizer links

• | Toe links

• | Upper control arms

• | Lower control arms

• | Trailing arms

• | Knuckles

• | Wheel bearing/hub

• | Shock absorbers