For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Speed Sensor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m(80 lb in)
2 | Rear Wheel Speed Sensor Clip (Qty: 4)
3 | Rear Wheel Speed Sensor

#### Procedure

1. Remove the nut from the wheel shield to get access.
2. Disconnect the speed sensor electrical connector.