For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedure

Disable the SIR system. Refer to SIR Disabling and Enabling.

1 | Front End Inflatable Restraint Discriminating Sensor Fastener

#### Procedure

1. Release the fastener from the front end inflatable restraint discriminating sensor.
2. Disconnect the electrical connector.

2 | Front End Inflatable Restraint Discriminating Sensor

#### Procedure

Push the front end inflatable restraint discriminating sensor to the left and pull it out from the front end upper tie bar.