For 1990-2009 cars

Caution: Use of harsh chemicals when cleaning can damage exterior lamps. Suggested cleaners are a mild soap and water, or Varnish Makers and Painters (VM&P) Naptha. VM&P Naptha is a specific type of naptha and should not be substituted by any other naptha.

The following components are attached to the body panels with adhesive tape.

The name plates.

In order to ensure a good replacement of new or old moldings, emblems and name plates, take the following precautions:

• | Warm the panel surface to between 21-32°C (70-90°F).

• | Clean the panels.

• | Remove any wax or oily film.

The following methods for attachment are listed:

Replacement nameplates.