For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the front floor console. Refer to Front Floor Console Replacement.

1 | Parking Brake Indicator Switch Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m(22 lb in)
2 | Parking Brake Indicator Switch

#### Procedure

Disconnect the electrical connector from the park brake indicator switch.