For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the General Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Note: Verify the vehicle suspension package RPO. Verify that the ride is too soft or too hard. Does the vehicle ride normally? | System OK | Go to Step 3
3 | Check the tire inflation and adjust to specifications. Refer to Vehicle Certification, Tire Placard, Anti-Theft, and Service Parts ID Label. Did you adjust the tire pressure? | Go to Step 6 | Go to Step 4
4 | Inspect the vehicle trim height. Refer to Trim Height Inspection. Did you find and correct the condition? | Go to Step 6 | Go to Step 5
5 | Inspect the following suspension components for wear or damage:

• | Shock Absorbers--Refer to Suspension Strut and Shock Absorber Testing - On Vehicle.

• | Springs

Did you find and correct the condition?

Go to Step 6

--

6 | Drive the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3