For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel lower center trim panel. Refer to Instrument Panel Lower Center Trim Panel Replacement.

1 | Radio Control Module Fastener (Qty: 5)

#### Procedure

1. Disconnect the radio control module electrical connector.
2. Disconnect antenna cable.
3. Use a flat bladed plastic trim tool to aid in the removal of the radio control module.

2 | Radio Control Module