For 1990-2009 cars

## Front Seat Tilt Adjuster Lever Replacement Driver or Passenger Seat 6-Way Hybrid

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove front seat tilt adjuster lever bolt cap. Refer to Front Seat Tilt Adjuster Lever Bolt Cap Replacement.

1 | Front Seat Tilt Adjuster Lever Bolt Cap
2 | Front Seat Tilt Adjuster Lever Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
3 | Front Seat Tilt Adjuster Lever

#### Procedure

Use a small flat-bladed tool to release the front seat tilt adjuster lever bolt cap.