For 1990-2009 cars

## Rear Object Sensor Wiring Harness Replacement 68HB

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.

1 | Rear Object Sensor Wiring Harness Retainer (Qty: 5)
2 | Rear Object Sensor Wiring Harness

#### Procedure

Disconnect the rear object sensor wiring harness electrical connector from the rear object sensors.