For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Brake system releases and returns to rest slowly; vehicle motion is hindered by brake system briefly after release of brake pedal.
1 | Were you sent here from the Hydraulic Brake Symptom table? | Go to Step 2 | Go to Symptoms - Hydraulic Brakes
2 |

1. Inspect the hydraulic brake system for the following conditions:

• | Improper operation of caliper pistons

• | Internally damaged flexible brake hoses; hindering brake release

• | Contaminated brake fluid

• | Damaged or improperly operating master cylinder

2. Adjust, repair or replace components as necessary. Refer to Hydraulic Brake System Diagnosis.

Did you find and correct a condition?

Go to Step 5

Go to Step 3

3 |

1. Inspect the brake assist system for the following conditions:

• | Binding, bent or damaged pedal pushrod, pedal, or pedal bracket

• | Damaged or improperly operating vacuum booster, if equipped

• | Damaged or improperly operating hydraulic booster, if equipped

2. Adjust, repair or replace components as necessary.

Did you find and correct a condition?

Go to Step 5

Go to Step 4

4 |

1. Inspect the disc brake system for the following conditions:

• | Damaged or excessively worn caliper hardware and/or lining hardware

• | Distorted or damaged linings

• | Lack of lubrication or excessive corrosion on metal to metal contact surfaces

• | Bent or damaged caliper or mounting component

2. Adjust, repair or replace components as necessary. Refer to Disc Brake System Diagnosis.

Did you find and correct a condition?

Go to Step 5

Go to Symptoms - Hydraulic Brakes

5 |

1. Install or connect components that were removed or disconnected during diagnosis.
2. Road test the vehicle in order to confirm proper operation. Refer to Brake System Vehicle Road Test.

Is the condition still present?

Go to Step 2

System OK