For 1990-2009 cars

## Driver or Passenger Seat Adjuster Handle Replacement 2/4-Way Hybrid, 6-Way Hybrid, 6-Way H

Callout | Component Name
--- | ---
1 | Driver or Passenger Seat Adjuster Handle Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

For removal of the driver or passenger seat adjuster handle move the front seat full backward.

Tighten
3.5 N·m (31 lb in)

2 | Driver or Passenger Seat Adjuster Handle