For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel lower trim panel - left side. Refer to LINK.

1 | Inner Electrical Center

#### Procedure

1. Disconnect the lower three electrical connectors on the body control module.
2. Clip out the inner electrical center.

2 | Body Control Module

#### Procedure

1. Disconnect the upper four electrical connectors on the body control module.
2. Pull out the body control module of the bracket.
3. For programming and set up information refer to Control Module References.