For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel lower trim panel - driver side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.

1 | Instrument Panel Lower Trim Panel Insulator Retainer (Qty: 2)
2 | Instrument Panel Lower Trim Panel Insulator

#### Procedure

Use BO-569-A plug lifter to release the retainer clips securing the insulator to the instrument panel.

#### Special Tools

BO-569-A Plug Lifter

For equivalent regional tools, refer to Special Tools.