For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Bumper Fascia Fastener (Qty: 6) Tip Reach underneath the wheelhouse to access the fastener.
2 | Front Bumper Fascia Fastener (Qty: 6)
3 | Front Bumper Fascia Plastic Retainer (Qty: 4)
4 | Front Bumper Fascia Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
5 | Front Bumper Fascia

#### Procedure

1. Disconnect any electrical connectors.
2. Transfer components as necessary.