For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the headlining trim panel.
2. Remove front wheelhouse liner. Refer to Front Wheelhouse Rear Liner Replacement.

1 | Sunroof Housing Front Drain Hose

#### Procedure

1. Remove the sunroof housing front drain hose from the sunroof assembly.
2. Remove the rubber grommet from the front wheelhouse.
3. Draw the front drain hose out of the a-pillar.
4. Separate the rubber grommet from the front drain hose.

Tip
It`s only necessary to lower the headlining trim panel in the front area.