For 1990-2009 cars

Name | AF-40-6
--- | ---
RPO Codes | M36&F46
Production Location | Japan
Vehicle Platform (Engine/Transmission) Usage | GE
1st Gear Ratio | 4.148
2nd Gear Ratio | 2.37
3rd Gear Ratio | 1.556
4th Gear Ratio | 1.155
5th Gear Ratio | 0.859
6th Gear Ratio | 0.686
Reverse | 3.394
Torque Converter Size (Diameter of Torque Converter Turbine) | 260 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | AW-1
Transmission Type: 6 | Six Forward Gears
Transmission Type: E | Electronic Controls
Position Quadrant | P, R, N, D
Case Material | Die Cast Aluminum
Transmission Weight Dry (Approximate) | AWD: 88.8 kg FWD: 88.5 kg
Transmission Weight Wet (Approximate) | AWD: 94.6 kg FWD: 94.3 kg