For 1990-2009 cars

## Front Bumper Fascia Support Replacement Left Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement

1 | Front Bumper Fascia Support Fastener (Qty: 2)
2 | Front Bumper Fascia Support Retainer
3 | Front Bumper Fascia Support

#### Procedure

Using a small flat-bladed tool, release the one outer locking retainer from the front bumper fascia outer bracket support.

## Front Bumper Fascia Support Replacement Right Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Fascia Bracket Support Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Bumper Fascia Bracket Support Retainer
3 | Front Bumper Fascia Bracket Support

#### Procedure

Using a small flat-bladed tool, release the one outer locking retainer from the front bumper fascia outer bracket support.