For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove sunroof air deflector cover. Refer to Sunroof Air Deflector Cover Replacement

1 | Sunroof Window Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Turn the ignition on.
2. Lift up the sunroof window to the vent position.
3. Slide the sunshade to the full rearward position.
4. Remove the sunroof air deflector cover left and right.
5. Remove the sunroof window fasteners on both sides.

Tighten
4 N·m (35 lb in)

2 | Sunroof Window

#### Procedure

After the installation adjust the sunroof window. Refer to Sunroof Window Height and Opening Fit Adjustment