For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame-To-Body Bolts | 160 N·m | 118 lb ft
Frame-To-Body Reinforcement Bolts | 60 N·m + 30-45 degrees | 44 lb ft + 30-45 degrees
Front Lower Control Arm Bushing Fastener | 40 N·m + 30 degrees | 30 lb ft + 30 degrees
Front Transmission Mount-To-Frame Bolt | 100 N·m | 74 lb ft
Rear Transmission Mount-To-Frame Bolt | 100 N·m | 74 lb ft
Stabilizer Shaft Link Fastener | 50 N·m | 37 lb ft
Stabilizer Shaft Insulator Fastener | 22 N·m + 30 degrees + 15 degrees | 16 lb ft + 30 degrees + 15 degrees
Steering Gear Fastener | 110 N·m + 150 degrees + 15 degrees | 81 lb ft + 150 degrees + 15 degrees