For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove sunroof window. Refer to Sunroof Window Replacement.
2. Remove sunroof sunshade motor. Refer to Sunroof Sunshade Motor Replacement.
3. Remove the sunroof module assembly. Refer to Sunroof Module Assembly Replacement.
4. Remove sunroof housing drain gutter. Refer to Sunroof Housing Drain Gutter Replacement.

1 | Sunroof Sunshade

1. Remove the 2 rear sunroof module assembly brackets.
2. Move the sunroof sunshade rearward out of the sliding rail.