For 1990-2009 cars

#### Special Tools

EN 46104 Water Pump Pulley Holding Tool

For equivalent regional tools, refer to Special Tools.

1. Install the EN 46104 holder (1) onto the water pump pulley.
2. Remove the water pump pulley bolts (1).
3. Remove the water pump pulley (2).
4. Remove the 6 water pump bolts (1).
5. Remove the water pump (2) from the front cover.
6. Remove the water pump gasket (3).