For 1990-2009 cars

## Base Engine Misfire with Coolant Consumption LDK

Cause | Correction
--- | ---
Faulty cylinder head gasket and/or cracking, or other damage to the cylinder head and engine block cooling system passages. Coolant consumption may or may not cause the engine to overheat. |

• | Inspect for spark plugs saturated by coolant.

• | Perform a cylinder leak down test.

• | Inspect the cylinder head and engine block for damage to the coolant passages and/or a faulty head gasket.

• | Repair or replace as required.