For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

1 | Front Wheelhouse Rear Liner Retainer

#### Procedure

Use a BO-569-A plug lifter to aid in the removal of the front wheelhouse rear liner.

#### Special Tools

BO-569-A Plug Lifter

For equivalent regional tools, refer to Special Tools.

2 | Front Wheelhouse Rear Liner