For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Pull Handle Cover
2 | Rear Side Door Handle Cover

#### Procedure

Pull handle back to remove cap. Use suitable tool to unsnap.

3 | Rear Side Door Inside Handle Fastener
4 | Rear Side Door Pull Handle Fastener (Qty: 2)
5 | Rear Side Door Trim Panel Retainer (Qty: 6)

#### Procedure

1. Use a BO-569-A plug lifter to aid in the removal of the door trim panel.
2. Pull upwards on the door lock retainer cable to disengage.

#### Special Tools

BO-569-A Plug Lifter

6 | Rear Side Door Trim Panel