For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Fender | 9 N·m | 79.7 lb in
Headlamp Mount Panel Outer Bracket | 9 N·m | 79.7 lb in
Front Side Door Check Link - Door Side | 9 N·m | 79.7 lb in
Front Side Door Check Link - Body Side | 22 N·m | 16.2 lb ft
Front Side Door - Door Side | 25 N·m | 18.4 lb ft
Front Side Door - Hinge | 25 N·m | 18.4 lb ft
Front Side Door Hinge | 22 N·m | 16.2 lb ft
Rear Side Door Check Link - Door Side | 9 N·m | 79.7 lb in
Rear Side Door Check Link - Body Side | 22 N·m | 16.2 lb ft
Rear Side Door - Door Side | 25 N·m | 18.4 lb ft
Rear Side Door - Hinge | 25 N·m | 18.4 lb ft
Rear Side Door Hinge | 22 N·m | 16.2 lb ft
Horn | 17 N·m | 12.5 lb ft
Hood | 9 N·m | 79.7 lb in
Hood Hinge | 9 N·m | 79.7 lb in
Hood Hinge Bracket | 22 N·m | 16.2 lb ft
Hood Front Bumper Bracket | 22 N·m | 16.2 lb ft
Rear Compartment Lid | 22 N·m | 16.2 lb ft
Rear Compartment Lid Hinge | 22 N·m | 16.2 lb ft
Rear Bumper Impact Bar | 40 N·m | 29.5 lb ft
Front End Upper Tie Bar | 22 N·m | 16.2 lb ft
Front Bumper Energy Absorber | 100 N·m | 73.7 lb ft