For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the plenum water deflector. Refer to Plenum Water Deflector Replacement.

1 | Windshield Wiper System Module Fastener (Qty: 3)
2 | Windshield Wiper System Module

#### Procedure

1. Disconnect the electrical connector from the wiper motor.
2. Carefully lift the windshield wiper system module out of the plenum.