For 1990-2009 cars

Cause | Action
--- | ---
DEFINITION: A rattle noise coming from the clutch components with the clutch disengaged or engaged. Review the Symptoms - Clutch and perform the necessary inspections.
Idle rattle clutch engaged | Replace the clutch disc, due to faulty dampener springs. Refer to Clutch Assembly Replacement.
Clutch is improperly installed | Remove the clutch and install it correctly. Refer to Clutch Assembly Replacement.
Clutch disc dampener worn or damaged |

1. Inspect the clutch disc for a broken or worn dampener.
2. Replace the clutch assembly. Refer to Clutch Assembly Replacement.

Clutch disc splines worn |

1. Inspect the clutch disc hub to input shaft splines for excessive clearance.
2. Replace the clutch assembly if the clutch splines are worn. Refer to Clutch Assembly Replacement.