For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Fuel Feed Pipe Connector

#### Procedure

1. Release the connector securing retainer.
2. Pull the pipe off the fuel feed to fuel rail pipe.

2 | Rear Fuel Feed Pipe Connector

#### Procedure

1. Release the connector securing retainer.
2. Pull the pipe off the fuel feed to fuel tank pipe.

3 | Fuel Feed Pipe Retainer (Qty 4)

#### Procedure

Release the fuel feed pipe from the underbody retainers.

4 | Fuel Feed Pipe