For 1990-2009 cars

## Rear License Plate Lamp Bulb Replacement Rear

Callout | Component Name
--- | ---
1 | Rear License Lamp Retainer Tip Using a small flat-bladed tool, pull the right side down out from the rear bumper fascia opening.
2 | Rear License Lamp Socket Tip Rotate the lamp socket counter clock wise and remove.
3 | Rear License Lamp Bulb Caution: Refer to Avoid Touching the Bulb Caution in the Preface section. Tip Service the bulb, as needed.